### - h -

- H : _ll_ecc_curve_init
- handle : ble_gattc_ntf_ind_t , ble_gattc_read_value_t , ble_gattc_write_t , ble_gatts_ntf_ind_t , gattc_browse_attr_char_t , gattc_write_attr_value_t , gattc_write_no_resp_t , gatts_noti_ind_t , gatts_prep_write_cfm_t , gatts_prep_write_req_cb_t , gatts_read_cfm_t , gatts_read_req_cb_t , gatts_write_cfm_t , gatts_write_req_cb_t , prf_att_info_t , read_multiple_t , rscs_c_evt_t
- handle_count : gattc_read_multiple_t
- handle_decl : ble_gattc_char_t
- handle_mode : app_gpiote_param_t
- handle_value : ble_gattc_char_t
- hba1c : gls_meas_ctx_t
- hci_subver : gap_dev_version_ind_t
- hci_ver : gap_dev_version_ind_t
- header_base : ags_ack_packet_t , ags_header_first_ext_t , ags_header_first_t , ags_header_subs_ext_t , ags_header_subs_t
- height : bcs_meas_val_t , uds_chars_val_t , wss_meas_val_t
- height_present : bcs_meas_flag_t , uds_chars_flag_t
- hid_info : hids_init_t
- hmac_done_callback : _hal_hmac_callback
- hmac_error_callback : _hal_hmac_callback
- hmac_mask : _keyram_mask
- hmac_msp_deinit : _hal_hmac_callback
- hmac_msp_init : _hal_hmac_callback
- host_subver : gap_dev_version_ind_t
- host_ver : gap_dev_version_ind_t
- hour : _calendar_alarm , _calendar_time , prf_date_time_t
- hours_since_update : cts_c_ref_time_info_t , cts_ref_time_info_t
- hperiod : pwm_init_t
- hprescaler : _ll_pwm_init_t
- hr_meas_buff : hrs_c_evt_t
- hr_value : hrs_c_hr_meas_t
- hrs_ctrl_point_handle : hrs_c_handles_t
- hrs_hr_meas_cccd_handle : hrs_c_handles_t
- hrs_hr_meas_handle : hrs_c_handles_t
- hrs_sensor_loc_handle : hrs_c_handles_t
- hrs_srvc_end_handle : hrs_c_handles_t
- hrs_srvc_start_handle : hrs_c_handles_t
- hw_flow_ctrl : _ll_uart_init_t , _uart_init
- hw_rev_str : dis_init_t