Data Fields
bcs_meas_flag_t Struct Reference
BLE Services » Body Composition Service (BCS) » Structures

Body composition Measurement flag data. More...

`#include <bcs.h>`

## Data Fields
uint8_t | time_stamp_present:1
uint8_t | user_id_present:1
uint8_t | basal_metabolism_present:1
uint8_t | muscle_percentage_present:1
uint8_t | muscle_mass_present:1
uint8_t | fat_free_mass_present:1
uint8_t | soft_lean_mass_present:1
uint8_t | body_water_mass_present:1
uint8_t | impedance_present:1
uint8_t | weight_present:1
uint8_t | height_present:1

## Detailed Description

Body composition Measurement flag data.

## Field Documentation

## ◆ basal_metabolism_present

uint8_t bcs_meas_flag_t::basal_metabolism_present

Basal Metabolism flag.

## ◆ body_water_mass_present

uint8_t bcs_meas_flag_t::body_water_mass_present

Body Water Mass flag.

## ◆ fat_free_mass_present

uint8_t bcs_meas_flag_t::fat_free_mass_present

Fat Free Mass flag.

## ◆ height_present

uint8_t bcs_meas_flag_t::height_present

Height flag.

## ◆ impedance_present

uint8_t bcs_meas_flag_t::impedance_present

Impedance flag.

## ◆ muscle_mass_present

uint8_t bcs_meas_flag_t::muscle_mass_present

Muscle Mass flag.

## ◆ muscle_percentage_present

uint8_t bcs_meas_flag_t::muscle_percentage_present

Muscle Percentage flag.

## ◆ soft_lean_mass_present

uint8_t bcs_meas_flag_t::soft_lean_mass_present

Soft Lean Mass flag.

## ◆ time_stamp_present

uint8_t bcs_meas_flag_t::time_stamp_present

Time Stamp flag.

## ◆ user_id_present

uint8_t bcs_meas_flag_t::user_id_present

User ID flag.

## ◆ weight_present

uint8_t bcs_meas_flag_t::weight_present

Weight flag.

The documentation for this struct was generated from the following file:

- bcs.h