Data Fields
ans_c_new_alert_t Struct Reference
BLE Services » Alert Notification Service Client (ANS_C) » Structures

Alert Notification Service Client decoded New Alert value. More...

`#include <ans_c.h>`

## Data Fields
ans_c_alert_cat_id_t | cat_id
uint8_t | alert_num
uint8_t | str_info [ANS_C_UTF_8_STR_LEN_MAX]
uint8_t | length

## Detailed Description

Alert Notification Service Client decoded New Alert value.

## Field Documentation

## ◆ alert_num

uint8_t ans_c_new_alert_t::alert_num

Number of new alert.

## ◆ cat_id

ans_c_alert_cat_id_t ans_c_new_alert_t::cat_id

Category ID.

## ◆ length

uint8_t ans_c_new_alert_t::length

Length of Text String.

## ◆ str_info

uint8_t ans_c_new_alert_t::str_info[ANS_C_UTF_8_STR_LEN_MAX]

Text String Information.

The documentation for this struct was generated from the following file:

- ans_c.h