Data Fields
gap_adv_second_cfg_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Management » Structures

Configuration for advertising on secondary channel. More...

`#include <ble_gapm.h>`

## Data Fields
uint8_t | max_skip
gap_le_phy_value_t | phy
uint8_t | adv_sid

## Detailed Description

Configuration for advertising on secondary channel.

## Field Documentation

## ◆ adv_sid

uint8_t gap_adv_second_cfg_t::adv_sid

Advertising SID. Allowed range is 0x00 to 0x0F.

## ◆ max_skip

uint8_t gap_adv_second_cfg_t::max_skip

Maximum number of advertising events the controller can skip before sending the AUX_ADV_IND packets. The range is 0x00 to 0xFF. 0x00 means that AUX_ADV_IND PDUs shall be sent prior to each advertising events.

## ◆ phy

gap_le_phy_value_t gap_adv_second_cfg_t::phy

Indicate on which PHY secondary advertising has to be performed. See enum gap_le_phy_value_t.

The documentation for this struct was generated from the following file:

- ble_gapm.h