Data Fields
ags_ack_packet_t Struct Reference
BLE Services » Alexa Gadget Service (AGS) » Structures

Alexa Gadget Service ACK packet. More...

`#include <ags.h>`

## Data Fields
ags_header_base_t | header_base
uint8_t | reserved_1
uint8_t | payload_length
uint8_t | reserved_2
uint8_t | result_code

## Detailed Description

Alexa Gadget Service ACK packet.

## Field Documentation

## ◆ header_base

ags_header_base_t ags_ack_packet_t::header_base

Header base.

## ◆ payload_length

uint8_t ags_ack_packet_t::payload_length

Length of the ACK packet.

## ◆ reserved_1

uint8_t ags_ack_packet_t::reserved_1

Reserved.

## ◆ reserved_2

uint8_t ags_ack_packet_t::reserved_2

Reserved.

## ◆ result_code

uint8_t ags_ack_packet_t::result_code

A result code, which depends on whether this is an ACK or a NACK. ags_header_ack_flag_t

The documentation for this struct was generated from the following file:

- ags.h