Data Fields
gap_peer_name_ind_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control » Structures

Name of peer device indication. More...

`#include <ble_gapc.h>`

## Data Fields
gap_addr_t | peer_addr
uint8_t | addr_type
uint8_t | name_len
uint8_t | name [__ARRAY_EMPTY]

## Detailed Description

Name of peer device indication.

## Field Documentation

## ◆ addr_type

uint8_t gap_peer_name_ind_t::addr_type

Peer device address type.

## ◆ name

uint8_t gap_peer_name_ind_t::name[__ARRAY_EMPTY]

Peer device name.

## ◆ name_len

uint8_t gap_peer_name_ind_t::name_len

Peer device name length.

## ◆ peer_addr

gap_addr_t gap_peer_name_ind_t::peer_addr

Peer device bd address.

The documentation for this struct was generated from the following file:

- ble_gapc.h