ble_services Directory Reference

## Files
file | ags.h [code]
| Alexa Gadgets Service API.
file | ancs_c.h [code]
| ANCS Service API.
file | ancs_protocol.h [code]
| ANCS Protocol API.
file | ans.h [code]
| Alert Notification Service API.
file | ans_c.h [code]
| Alert Notification Service Client API.
file | bas.h [code]
| Battery Service API.
file | bas_c.h [code]
| Battery Service Client API.
file | bcs.h [code]
| Body Composition Service API.
file | ble_prf_types.h [code]
| Profile/Service Common Types.
file | ble_prf_utils.h [code]
| Profile/Service Utilities API.
file | ble_srv_disc_utils.h [code]
| Service Discovery Utilities API.
file | bps.h [code]
| Blood Pressure Service API.
file | cscs.h [code]
| Cycling Speed and Cadence Service API.
file | cts.h [code]
| Current Time Service API.
file | cts_c.h [code]
| Current Time Service Client API.
file | dis.h [code]
| Device Information Service API.
file | dis_c.h [code]
| Device Information Service Client API.
file | dss.h [code]
| Device Synchronize Service API.
file | escs.h [code]
| Eddystone Configuration Service API.
file | fast_otas.h [code]
| FAST_OTA Service API.
file | gls.h [code]
| Glucose Service API.
file | gls_db.h [code]
| Glucose Service Database API.
file | gls_racp.h [code]
| Glucose Service Record Access Control Point API.
file | gus.h [code]
| Goodix UART Service API.
file | gus_c.h [code]
| Header file - Goodix UART Service Client.
file | hids.h [code]
| Human Interface Device Service API.
file | hrrcps.h [code]
| HRS RSCS Relay Control Point Service API.
file | hrs.h [code]
| Heart Rate Service API.
file | hrs_c.h [code]
| Heart Rate Service Client API.
file | hts.h [code]
| Health Thermometer Service API.
file | ias.h [code]
| Immediate Alarm Service API.
file | ias_c.h [code]
| Immediate Alert Service Client API.
file | lls.h [code]
| Link Loss Service API.
file | lls_c.h [code]
| Link Loss Service Client API.
file | lns.h [code]
| Log Notification Service API.
file | mlmr.h [code]
| Goodix UART Service API.
file | mlmr_c.h [code]
| Header file - Goodix UART Service Client.
file | ndcs.h [code]
| Next DST Change Service API.
file | otas.h [code]
| OTA Service API.
file | otas_c.h [code]
| OTAS Client API.
file | pass.h [code]
| Phone Alert Status Service API.
file | pass_c.h [code]
| API.
file | pcs.h [code]
| Power Consumption Service API.
file | rscs.h [code]
| Running Speed and Cadence Service API.
file | rscs_c.h [code]
| Running Speed and Cadence Service Client API.
file | rtus.h [code]
| Reference Time Update Service API.
file | sample_service.h [code]
| Header file - sample_profile Server Role.
file | ths.h [code]
| Throughput Service API.
file | ths_c.h [code]
| Throughput Client API.
file | thscps.h [code]
| Throughput Control Point Service API.
file | tps.h [code]
| Tx Power Service API.
file | tps_c.h [code]
| Tx Power Service Client API.
file | uds.h [code]
| User Data Service API.
file | wechat.h [code]
| WeChat Service API.
file | wss.h [code]
| Weight Scale Service API.