Macros
SPI Flags Definition
Peripheral Driver » HAL Driver » SPI » Defines » SPI Exported Constants

## Macros
#define | SPI_FLAG_DCOL LL_SSI_SR_DCOL
#define | SPI_FLAG_TXE LL_SSI_SR_TXE
#define | SPI_FLAG_RFF LL_SSI_SR_RFF
#define | SPI_FLAG_RFNE LL_SSI_SR_RFNE
#define | SPI_FLAG_TFE LL_SSI_SR_TFE
#define | SPI_FLAG_TFNF LL_SSI_SR_TFNF
#define | SPI_FLAG_BUSY LL_SSI_SR_BUSY

## Detailed Description

## Macro Definition Documentation

## ◆ SPI_FLAG_BUSY

#define SPI_FLAG_BUSY LL_SSI_SR_BUSY

Busy flag

## ◆ SPI_FLAG_DCOL

#define SPI_FLAG_DCOL LL_SSI_SR_DCOL

Data collision error flag

## ◆ SPI_FLAG_RFF

#define SPI_FLAG_RFF LL_SSI_SR_RFF

Rx FIFO full flag

## ◆ SPI_FLAG_RFNE

#define SPI_FLAG_RFNE LL_SSI_SR_RFNE

Rx FIFO not empty flag

## ◆ SPI_FLAG_TFE

#define SPI_FLAG_TFE LL_SSI_SR_TFE

Tx FIFO empty flag

## ◆ SPI_FLAG_TFNF

#define SPI_FLAG_TFNF LL_SSI_SR_TFNF

Tx FIFO not full flag

## ◆ SPI_FLAG_TXE

#define SPI_FLAG_TXE LL_SSI_SR_TXE

Transmission error flag