Macros
GAP PHY OPTIONS (bitmask)
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control » Defines

## Macros
#define | PHY_OPT_NO_CODING 0x00
| The Host has no preferred coding when transmitting on the LE Coded PHY. More...
#define | PHY_OPT_S2_CODING 0x01
| The Host prefers that S=2 coding be used when transmitting on the LE Coded PHY. More...
#define | PHY_OPT_S8_CODING 0x02
| The Host prefers that S=8 coding be used when transmitting on the LE Coded PHY. More...

## Detailed Description

## Macro Definition Documentation

## ◆ PHY_OPT_NO_CODING

#define PHY_OPT_NO_CODING 0x00

The Host has no preferred coding when transmitting on the LE Coded PHY.

Definition at line 81 of file ble_gapc.h.

## ◆ PHY_OPT_S2_CODING

#define PHY_OPT_S2_CODING 0x01

The Host prefers that S=2 coding be used when transmitting on the LE Coded PHY.

Definition at line 82 of file ble_gapc.h.

## ◆ PHY_OPT_S8_CODING

#define PHY_OPT_S8_CODING 0x02

The Host prefers that S=8 coding be used when transmitting on the LE Coded PHY.

Definition at line 83 of file ble_gapc.h.