Macros
InitStrcut default configuartion
Peripheral Driver » LL Driver » XQSPI » Defines » XQSPI Exported Constants

## Macros
#define | LL_XQSPI_DEFAULT_CONFIG
| LL XQSPI InitStrcut default configuartion. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_XQSPI_DEFAULT_CONFIG

#define LL_XQSPI_DEFAULT_CONFIG

Value:
{ \
.mode = LL_XQSPI_MODE_QSPI, \
.cache_mode = LL_XQSPI_CACHE_EN, \
.read_cmd = LL_XQSPI_XIP_CMD_READ, \
.data_size = LL_XQSPI_QSPI_DATASIZE_8BIT, \
.data_order = LL_XQSPI_QSPI_MSB, \
.clock_polarity = LL_XQSPI_SCPOL_HIGH, \
.clock_phase = LL_XQSPI_SCPHA_2EDGE, \
.baud_rate = LL_XQSPI_BAUD_RATE_16M, \
}

LL XQSPI InitStrcut default configuartion.

Definition at line 307 of file gr55xx_ll_xqspi.h.

LL_XQSPI_MODE_QSPI
#define LL_XQSPI_MODE_QSPI
QSPI mode
Definition: gr55xx_ll_xqspi.h:136
LL_XQSPI_SCPOL_HIGH
#define LL_XQSPI_SCPOL_HIGH
Clock to 1 when idle.
Definition: gr55xx_ll_xqspi.h:273
LL_XQSPI_QSPI_MSB
#define LL_XQSPI_QSPI_MSB
MSB first for transfer.
Definition: gr55xx_ll_xqspi.h:246
LL_XQSPI_BAUD_RATE_16M
#define LL_XQSPI_BAUD_RATE_16M
Clock to 16MHz.
Definition: gr55xx_ll_xqspi.h:283
LL_XQSPI_CACHE_EN
#define LL_XQSPI_CACHE_EN
Cache ON
Definition: gr55xx_ll_xqspi.h:177
LL_XQSPI_QSPI_DATASIZE_8BIT
#define LL_XQSPI_QSPI_DATASIZE_8BIT
Data length for XQSPI transfer: 8 bits.
Definition: gr55xx_ll_xqspi.h:253
LL_XQSPI_XIP_CMD_READ
#define LL_XQSPI_XIP_CMD_READ
Read mode
Definition: gr55xx_ll_xqspi.h:142
LL_XQSPI_SCPHA_2EDGE
#define LL_XQSPI_SCPHA_2EDGE
Second clock transition is the first data capture edge.
Definition: gr55xx_ll_xqspi.h:266