Public Attributes | List of all members
app_gpiote_param_t Struct Reference
Peripheral Driver » APP DRIVER » GPIO INTERRUPT » Structures

GPIOTE Interrupt parameters structure definition. More...

`#include <app_gpiote.h>`

## Public Attributes
app_io_type_t | type
| Specifies IO type. More...
uint32_t | pin
| Specifies the IO pins to be configured. More...
app_io_mode_t | mode
| Specifies the IO mode for the selected pins. More...
app_io_pull_t | pull
| Specifies the Pull-up or Pull-Down activation for the selected pins. More...
app_handle_mode_t | handle_mode
| Specifies the IO wakeup mode. More...
app_io_callback_t | io_evt_cb
| IO callback function. More...

## Detailed Description

GPIOTE Interrupt parameters structure definition.

Definition at line 85 of file app_gpiote.h.

## Member Data Documentation

## ◆ handle_mode

app_handle_mode_t app_gpiote_param_t::handle_mode

Specifies the IO wakeup mode.

Definition at line 91 of file app_gpiote.h.

## ◆ io_evt_cb

app_io_callback_t app_gpiote_param_t::io_evt_cb

IO callback function.

Definition at line 92 of file app_gpiote.h.

## ◆ mode

app_io_mode_t app_gpiote_param_t::mode

Specifies the IO mode for the selected pins.

Definition at line 89 of file app_gpiote.h.

## ◆ pin

uint32_t app_gpiote_param_t::pin

Specifies the IO pins to be configured.

Definition at line 88 of file app_gpiote.h.

## ◆ pull

app_io_pull_t app_gpiote_param_t::pull

Specifies the Pull-up or Pull-Down activation for the selected pins.

Definition at line 90 of file app_gpiote.h.

## ◆ type

app_io_type_t app_gpiote_param_t::type

Specifies IO type.

Definition at line 87 of file app_gpiote.h.

The documentation for this struct was generated from the following file:

- app_gpiote.h