Public Attributes | List of all members
hrs_c_hr_meas_t Struct Reference
BLE Services » Heart Rate Service Client (HRS_C) » Structures

Heart Rate Measurement characteristic value structure. More...

`#include <hrs_c.h>`

## Public Attributes
bool | is_sensor_contact_detected
| True if sensor contact has been detected. More...
uint16_t | hr_value
| Heart Rate Value. More...
uint8_t | rr_intervals_num
| Number of RR intervals. More...
float | rr_intervals [HRS_C_RR_INTERVALS_NUM_MAX]
| RR intervals. More...
uint16_t | energy_expended
| The accumulated energy expended in kilo Joules since the last time it was reset. More...

## Detailed Description

Heart Rate Measurement characteristic value structure.

Definition at line 123 of file hrs_c.h.

## Member Data Documentation

## ◆ energy_expended

uint16_t hrs_c_hr_meas_t::energy_expended

The accumulated energy expended in kilo Joules since the last time it was reset.

Definition at line 129 of file hrs_c.h.

## ◆ hr_value

uint16_t hrs_c_hr_meas_t::hr_value

Heart Rate Value.

Definition at line 126 of file hrs_c.h.

## ◆ is_sensor_contact_detected

bool hrs_c_hr_meas_t::is_sensor_contact_detected

True if sensor contact has been detected.

Definition at line 125 of file hrs_c.h.

## ◆ rr_intervals

float hrs_c_hr_meas_t::rr_intervals[HRS_C_RR_INTERVALS_NUM_MAX]

RR intervals.

Definition at line 128 of file hrs_c.h.

## ◆ rr_intervals_num

uint8_t hrs_c_hr_meas_t::rr_intervals_num

Number of RR intervals.

Definition at line 127 of file hrs_c.h.

The documentation for this struct was generated from the following file:

- hrs_c.h