Classes | Typedefs | Enumerations | Variables
Typedefs
SYSTEM » Power Manager

## Classes
struct | pwr_mgmt_var_box_t
| power manager setting parameter. More...
struct | pwr_table_t
| parameter configuration table. More...

## Typedefs
typedef void(* | trace_func_t) (uint8_t)
| Trace function type. More...
typedef void(* | periph_func_t) (void)
| Peripheral function type. More...
typedef void(* | pwr_before_sleep_func_t) (void)
| Before sleep function type. More...
typedef pwr_mgmt_dev_state_t(* | pwr_dev_check_func_t) (void)
| Device check function type. More...
typedef void(* | io_dump_func_t) (void)
| function registered to dump io configuration. More...
typedef void(* | mem_check_proc_t) (void)
| mem check process type. More...

## Enumerations
enum | boot_mode_t { COLD_BOOT = 0, WARM_BOOT }
| power manager boot type. More...
enum | pwr_mgmt_mode_t { PMR_MGMT_ACTIVE_MODE = 0x0, PMR_MGMT_IDLE_MODE, PMR_MGMT_SLEEP_MODE }
| power manager model. More...
enum | pwr_mgmt_dev_state_t { DEVICE_BUSY = 0x0, DEVICE_IDLE }
| power manager device work state. More...
enum | notify_timer_event_t { EVENT_APP_TIMER_START = 0, EVENT_APP_TIMER_STOP }
| power manager app timer work state. More...
enum | { AMS_PLAYER_ATTR_ID_NAME, AMS_PLAYER_ATTR_ID_PLAYBACK_INFO, AMS_PLAYER_ATTR_ID_VOLUME, IAS_ALERT_NONE, IAS_ALERT_MILD, IAS_ALERT_HIGH, TRC_PWR_WFE_MODE = 0, TRC_PWR_DSLEEP_MODE, TRC_PWR_ACTIVE_MODE, TRC_PWR_BLE_RET_DSLEEP, TRC_PWR_APP_TIMER_REFUSE, TRC_PWR_APP_TIMER_PASS, TRC_PWR_BLE_TIMER_PASS }
| PMU Tracking. More...

## Variables
pwr_table_t | pwr_table []
| pwr table. More...

## Detailed Description

## Typedef Documentation

## ◆ io_dump_func_t

typedef void(* io_dump_func_t) (void)

function registered to dump io configuration.

Definition at line 145 of file gr55xx_pwr.h.

## ◆ mem_check_proc_t

typedef void(* mem_check_proc_t) (void)

mem check process type.

Definition at line 148 of file gr55xx_pwr.h.

## ◆ periph_func_t

typedef void(* periph_func_t) (void)

Peripheral function type.

Definition at line 136 of file gr55xx_pwr.h.

## ◆ pwr_before_sleep_func_t

typedef void(* pwr_before_sleep_func_t) (void)

Before sleep function type.

Definition at line 139 of file gr55xx_pwr.h.

## ◆ pwr_dev_check_func_t

typedef pwr_mgmt_dev_state_t(* pwr_dev_check_func_t) (void)

Device check function type.

Definition at line 142 of file gr55xx_pwr.h.

## ◆ trace_func_t

typedef void(* trace_func_t) (uint8_t)

Trace function type.

Definition at line 133 of file gr55xx_pwr.h.

## Enumeration Type Documentation

## ◆ anonymous enum

anonymous enum

PMU Tracking.

Enumerator
AMS_PLAYER_ATTR_ID_NAME | Player attribute index of name.
AMS_PLAYER_ATTR_ID_PLAYBACK_INFO | Player attribute index of playback information.
AMS_PLAYER_ATTR_ID_VOLUME | Player attribute index of volume.
IAS_ALERT_NONE | No alert.
IAS_ALERT_MILD | Mild alert.
IAS_ALERT_HIGH | High alert.
TRC_PWR_WFE_MODE | WFE mode.
TRC_PWR_DSLEEP_MODE | Deep sleep mode.
TRC_PWR_ACTIVE_MODE | Active mode.
TRC_PWR_BLE_RET_DSLEEP | BLE return deep sleep.
TRC_PWR_APP_TIMER_REFUSE | App timer refuse.
TRC_PWR_APP_TIMER_PASS | App timer pass.
TRC_PWR_BLE_TIMER_PASS | BLE timer pass.

Definition at line 108 of file gr55xx_pwr.h.

## ◆ boot_mode_t

enum boot_mode_t

power manager boot type.

Enumerator
COLD_BOOT | Cold boot state.
WARM_BOOT | Warm boot state.

Definition at line 79 of file gr55xx_pwr.h.

## ◆ notify_timer_event_t

enum notify_timer_event_t

power manager app timer work state.

Enumerator
EVENT_APP_TIMER_START | App-timer start state.
EVENT_APP_TIMER_STOP | App-timer stop state.

Definition at line 101 of file gr55xx_pwr.h.

## ◆ pwr_mgmt_dev_state_t

enum pwr_mgmt_dev_state_t

power manager device work state.

Enumerator
DEVICE_BUSY | Device busy state.
DEVICE_IDLE | Device idle state.

Definition at line 94 of file gr55xx_pwr.h.

## ◆ pwr_mgmt_mode_t

enum pwr_mgmt_mode_t

power manager model.

Enumerator
PMR_MGMT_ACTIVE_MODE | Full speed state.
PMR_MGMT_IDLE_MODE | Idle state.
PMR_MGMT_SLEEP_MODE | Deep sleep state.

Definition at line 86 of file gr55xx_pwr.h.

## Variable Documentation

## ◆ pwr_table

pwr_table_t pwr_table[]
| extern

pwr table.