Macros
UART Line Error Flag Mask
Peripheral Driver » HAL Driver » UART » Defines » UART Exported Constants

## Macros
#define | UART_LINE_ERROR_MASK (LL_UART_LSR_PE | LL_UART_LSR_OE | LL_UART_LSR_FE | LL_UART_LSR_BI)
| UART interruptions flags mask. More...

## Detailed Description

## Macro Definition Documentation

## ◆ UART_LINE_ERROR_MASK

#define UART_LINE_ERROR_MASK (LL_UART_LSR_PE | LL_UART_LSR_OE | LL_UART_LSR_FE | LL_UART_LSR_BI)

UART interruptions flags mask.

Definition at line 311 of file gr55xx_hal_uart.h.