Macros
ADC Input Mode
Peripheral Driver » LL Driver » ADC » Defines » ADC Exported Constants

## Macros
#define | LL_ADC_INPUT_SINGLE (1UL << AON_SNSADC_CFG_SINGLE_EN_Pos)
| Single ended mode. More...
#define | LL_ADC_INPUT_DIFFERENTIAL (0x00000000UL)
| Differential mode. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_ADC_INPUT_DIFFERENTIAL

#define LL_ADC_INPUT_DIFFERENTIAL (0x00000000UL)

Differential mode.

Definition at line 148 of file gr55xx_ll_adc.h.

## ◆ LL_ADC_INPUT_SINGLE

#define LL_ADC_INPUT_SINGLE (1UL << AON_SNSADC_CFG_SINGLE_EN_Pos)

Single ended mode.

Definition at line 147 of file gr55xx_ll_adc.h.