Modules | Macros
Defines
BLE Services » Running Speed and Cadence Service Client (RSCS_C)

## Modules
| Measurement Flag Bits
| Running Speed and Cadence Measurement Flags.
| Feature Bits
| Running Speed and Cadence Service feature bits.

## Macros
#define | RSCS_C_CONNECTION_MAX
| Maximum number of HRS Client connections. More...
#define | RSCS_C_PT_RSP_LEN_MAX (3 + RSCS_C_SENSOR_LOC_SUP_NB)
| Maximum length of SC Control Point response value. More...
#define | RSCS_C_ERROR_PROC_IN_PROGRESS 0x80
| Error code: A previously triggered SC Control Point operation is still in progress. More...
#define | RSCS_C_ERROR_CCCD_INVALID 0x81
| Error code: The Client Characteristic Configuration descriptor is not configured. More...

## Detailed Description

## Macro Definition Documentation

## ◆ RSCS_C_CONNECTION_MAX

#define RSCS_C_CONNECTION_MAX

Value:
(10 < CFG_MAX_CONNECTIONS ?\
10 : CFG_MAX_CONNECTIONS)

Maximum number of HRS Client connections.

Definition at line 73 of file rscs_c.h.

## ◆ RSCS_C_ERROR_CCCD_INVALID

#define RSCS_C_ERROR_CCCD_INVALID 0x81

Error code: The Client Characteristic Configuration descriptor is not configured.

Definition at line 76 of file rscs_c.h.

## ◆ RSCS_C_ERROR_PROC_IN_PROGRESS

#define RSCS_C_ERROR_PROC_IN_PROGRESS 0x80

Error code: A previously triggered SC Control Point operation is still in progress.

Definition at line 75 of file rscs_c.h.

## ◆ RSCS_C_PT_RSP_LEN_MAX

#define RSCS_C_PT_RSP_LEN_MAX (3 + RSCS_C_SENSOR_LOC_SUP_NB)

Maximum length of SC Control Point response value.

Definition at line 74 of file rscs_c.h.