Macros
QSPI Instruction and Address Mode
Peripheral Driver » HAL Driver » QSPI » Defines » QSPI Exported Constants

## Macros
#define | QSPI_INST_ADDR_ALL_IN_SPI LL_SSI_INST_ADDR_ALL_IN_SPI
| Instruction and address are sent in SPI mode. More...
#define | QSPI_INST_IN_SPI_ADDR_IN_SPIFRF LL_SSI_INST_IN_SPI_ADDR_IN_SPIFRF
| Instruction is sent in SPI mode, and address is sent in Daul/Quad SPI mode. More...
#define | QSPI_INST_ADDR_ALL_IN_SPIFRF LL_SSI_INST_ADDR_ALL_IN_SPIFRF
| Instruction and address are sent in Daul/Quad SPI mode. More...

## Detailed Description

## Macro Definition Documentation

## ◆ QSPI_INST_ADDR_ALL_IN_SPI

#define QSPI_INST_ADDR_ALL_IN_SPI LL_SSI_INST_ADDR_ALL_IN_SPI

Instruction and address are sent in SPI mode.

Definition at line 330 of file gr55xx_hal_qspi.h.

## ◆ QSPI_INST_ADDR_ALL_IN_SPIFRF

#define QSPI_INST_ADDR_ALL_IN_SPIFRF LL_SSI_INST_ADDR_ALL_IN_SPIFRF

Instruction and address are sent in Daul/Quad SPI mode.

Definition at line 332 of file gr55xx_hal_qspi.h.

## ◆ QSPI_INST_IN_SPI_ADDR_IN_SPIFRF

#define QSPI_INST_IN_SPI_ADDR_IN_SPIFRF LL_SSI_INST_IN_SPI_ADDR_IN_SPIFRF

Instruction is sent in SPI mode, and address is sent in Daul/Quad SPI mode.

Definition at line 331 of file gr55xx_hal_qspi.h.