Macros
Attribute and Service UUID Type
BLE » Generic Attribute Profile (GATT) » Generic Attribute Profile (GATT) Server » Defines

## Macros
#define | UUID_TYPE_16 (0x00)
| 16-bit UUID length. More...
#define | UUID_TYPE_128 (0x02)
| 128-bit UUID length. More...

## Detailed Description

## Macro Definition Documentation

## ◆ UUID_TYPE_128

#define UUID_TYPE_128 (0x02)

128-bit UUID length.

Parameter of SRVC_UUID_TYPE_SET, ATT_UUID_TYPE_SET.

Definition at line 115 of file ble_gatts.h.

## ◆ UUID_TYPE_16

#define UUID_TYPE_16 (0x00)

16-bit UUID length.

Parameter of SRVC_UUID_TYPE_SET, ATT_UUID_TYPE_SET.

Definition at line 114 of file ble_gatts.h.