Public Attributes | List of all members
ans_init_t Struct Reference
BLE Services » Alert Notification Service (ANS) » Structures

Alert Notification Service init stucture. More...

`#include <ans.h>`

## Public Attributes
ans_evt_handler_t | evt_handler
| Phone Alert Status Service event handler. More...
uint16_t | sup_new_alert_cat
| Initial mask of Supported New Alert Category. More...
uint16_t | sup_unread_alert_sta
| Initial mask of Unread Alert Status. More...

## Detailed Description

Alert Notification Service init stucture.

This contains all options and data needed for initialization of the service.

Definition at line 193 of file ans.h.

## Member Data Documentation

## ◆ evt_handler

ans_evt_handler_t ans_init_t::evt_handler

Phone Alert Status Service event handler.

Definition at line 195 of file ans.h.

## ◆ sup_new_alert_cat

uint16_t ans_init_t::sup_new_alert_cat

Initial mask of Supported New Alert Category.

Definition at line 196 of file ans.h.

## ◆ sup_unread_alert_sta

uint16_t ans_init_t::sup_unread_alert_sta

Initial mask of Unread Alert Status.

Definition at line 197 of file ans.h.

The documentation for this struct was generated from the following file:

- ans.h