Classes | Macros | Typedefs | Enumerations | Functions
ams_c.h File Reference
`#include "gr55xx_sys.h"`
`#include "ble_prf_types.h"`
`#include "custom_config.h"`

Go to the source code of this file.

## Classes
struct | ams_c_ett_attr_id_t
| Structure that stores the attribute to be concerned or to display completely. More...
struct | ams_c_cmd_list_t
| Structure that stores new command list. More...
struct | ams_c_attr_info_t
| Structure that stores attribute information. More...
struct | ams_c_cplt_attr_data_t
| Complete attribution's value . More...
struct | ams_c_handles_t
| Handles on the connected peer device needed to interact with it. More...
struct | ams_c_evt_t
| Apple Media Service Client event. More...

## Macros
#define | AMS_C_CONNECTION_MAX
| Maximum number of HRS Client connections. More...
#define | AMS_C_ATTR_COUNT_MAX 256
| The buffer size of command. More...
#define | AMS_C_TRUNCATED_FLAG (0x01<<0)
| Bit of truncated. More...
#define | AMS_SRVC_UUID
| UUID of Apple media service. More...
#define | AMS_CMD_UUID
| UUID of remote command. More...
#define | AMS_ATTR_UPDATE_UUID
| UUID of attribute update. More...
#define | AMS_ATTR_DISPLAY_UUID
| UUID of attribute display. More...

## Typedefs
typedef void(* | ams_c_evt_handler_t) (ams_c_evt_t *p_evt)
| Apple Media Service Client event handler type. More...

## Enumerations
enum | ams_c_cmd_id_t { AMS_CMD_ID_PLAY, AMS_CMD_ID_PAUSE, AMS_CMD_ID_TOGGLE_PLAY_PAUSE, AMS_CMD_ID_NEXT_TRACK, AMS_CMD_ID_PREVIOUS_TRACK, AMS_CMD_ID_VOLUME_UP, AMS_CMD_ID_VOLUME_DOWN, AMS_CMD_ID_ADVANCE_REPEAT_MODE, AMS_CMD_ID_ADVANCE_SHUFFLE_MODE, AMS_CMD_ID_SKIP_FORWARD, AMS_CMD_ID_SKIP_BACKWARD, AMS_CMD_ID_LIKE_TRACK, AMS_CMD_ID_DISLIKE_TRACK, AMS_CMD_ID_BOOK_MARK_TRACK }
| Apple Media Service Command ID. More...
enum | ams_c_ett_id_t { AMS_ETT_ID_PLAYER, AMS_ETT_ID_QUEUE, AMS_ETT_ID_TRACK }
| Apple Media Service entities index. More...
enum | { AMS_PLAYER_ATTR_ID_NAME, AMS_PLAYER_ATTR_ID_PLAYBACK_INFO, AMS_PLAYER_ATTR_ID_VOLUME, IAS_ALERT_NONE, IAS_ALERT_MILD, IAS_ALERT_HIGH, TRC_PWR_WFE_MODE = 0, TRC_PWR_DSLEEP_MODE, TRC_PWR_ACTIVE_MODE, TRC_PWR_BLE_RET_DSLEEP, TRC_PWR_APP_TIMER_REFUSE, TRC_PWR_APP_TIMER_PASS, TRC_PWR_BLE_TIMER_PASS }
| Apple Media Service player attribute index. More...
enum | { AMS_QUEUE_ATTR_ID_INDEX, AMS_QUEUE_ATTR_ID_COUNT, AMS_QUEUE_ATTR_ID_SHUFFLE_MODE, AMS_QUEUE_ATTR_ID_REPEAT_MODE }
| Apple Media Service queue attribute index. More...
enum | { AMS_TRACK_ATTR_ID_ARTIST, AMS_TRACK_ATTR_ID_ALBUM, AMS_TRACK_ATTR_ID_TITTLE, AMS_TRACK_ATTR_ID_DURATION }
| Apple Media Service track attribute index. More...
enum | ams_c_evt_type_t { AMS_C_EVT_INVALID, AMS_C_EVT_DISCOVERY_CPLT, AMS_C_EVT_DISCOVERY_FAIL, AMS_C_EVT_CMD_SEND_SUCCESS, AMS_C_EVT_CMD_UPDATE_RECEIVE, AMS_C_EVT_CMD_UPDATE_NTF_SET_SUCCESS, AMS_C_EVT_ATTR_FOCUS_SET_SUCCESS, AMS_C_EVT_ATTR_UPDATE_RECEIVE, AMS_C_EVT_ATTR_UPDATE_NTF_SET_SUCCESS, AMS_C_EVT_CPLT_ATTR_DISPLAY_SET_SUCCESS, AMS_C_EVT_CPLT_ATTR_READ_RSP, AMS_C_EVT_WRITE_OP_ERR }
| Apple Media Service Client Event type. More...

## Functions
sdk_err_t | ams_c_client_init (ams_c_evt_handler_t evt_handler)
| Register AMS Client event handler. More...
sdk_err_t | ams_c_disc_srvc_start (uint8_t conn_idx)
| Discover Apple Media Service on peer. More...
sdk_err_t | ams_c_cmd_notify_set (uint8_t conn_idx, bool is_enable)
| Enable or disable peer new command list notify. More...
sdk_err_t | ams_c_attr_update_notify_set (uint8_t conn_idx, bool is_enable)
| Enable or disable peer updated attribute notify. More...
sdk_err_t | ams_c_cplt_attr_read (uint8_t conn_idx)
| Read complete value of updated attrbute . More...
sdk_err_t | ams_c_cmd_send (uint8_t conn_idx, uint8_t cmd_id)
| Send command to peer device. More...
sdk_err_t | ams_c_attr_focus_set (uint8_t conn_idx, const ams_c_ett_attr_id_t *p_ett_attr_id)
| Set concerned attribute. More...
sdk_err_t | ams_c_attr_display_set (uint8_t conn_idx, const ams_c_attr_info_t *p_attr_info)
| Set the attribute that needs to be completely displayed. More...
bool | ams_c_cmd_enable_check (ams_c_cmd_id_t cmd_id)
| Check if the command is available. More...