Enumerations
Enumerations
BLE Services » Heart Rate Service Client (HRS_C)

## Enumerations
enum | hrs_c_evt_type_t { HRS_C_EVT_INVALID, HRS_C_EVT_DISCOVERY_COMPLETE, HRS_C_EVT_DISCOVERY_FAIL, HRS_C_EVT_HR_MEAS_NTF_SET_SUCCESS, HRS_C_EVT_HR_MEAS_VAL_RECEIVE, HRS_C_EVT_SENSOR_LOC_READ_RSP, HRS_C_EVT_CTRL_POINT_SET, HRS_C_EVT_WRITE_OP_ERR }
| Heart Rate Service Client event type. More...
enum | hrs_c_flag_bit_t { HRS_C_BIT_RATE_FORMAT = 0x01, HRS_C_BIT_SENSOR_CONTACT_DETECTED = 0x02, HRS_C_BIT_SENSOR_CONTACT_SUPPORTED = 0x04, HRS_C_BIT_ENERGY_EXPENDED_STATUS = 0x08, HRS_C_BIT_INTERVAL = 0x10 }
| Heart Rate Service Measurement flag bit. More...
enum | hrs_c_sensor_loc_t { HRS_C_SENS_LOC_OTHER, HRS_C_SENS_LOC_CHEST, HRS_C_SENS_LOC_WRIST, HRS_C_SENS_LOC_FINGER, HRS_C_SENS_LOC_HAND, HRS_C_SENS_LOC_EARLOBE, HRS_C_SENS_LOC_FOOT }
| Values for sensor location. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ hrs_c_evt_type_t

enum hrs_c_evt_type_t

Heart Rate Service Client event type.

Enumerator
HRS_C_EVT_INVALID | HRS Client invalid event.
HRS_C_EVT_DISCOVERY_COMPLETE | HRS Client has found HRS service and its characteristics.
HRS_C_EVT_DISCOVERY_FAIL | HRS Client found HRS service failed because of invalid operation or no found at the peer.
HRS_C_EVT_HR_MEAS_NTF_SET_SUCCESS | HRS Client has set Notification of Heart Rate Measure characteristic.
HRS_C_EVT_HR_MEAS_VAL_RECEIVE | HRS Client has received Heart Rate Measure value notification from peer.
HRS_C_EVT_SENSOR_LOC_READ_RSP | HRS Client has received Sensor Location Value read response.
HRS_C_EVT_CTRL_POINT_SET | HRS Client has set Control Point completely.
HRS_C_EVT_WRITE_OP_ERR | Error occured when HRS Client writen to peer.

Definition at line 82 of file hrs_c.h.

## ◆ hrs_c_flag_bit_t

enum hrs_c_flag_bit_t

Heart Rate Service Measurement flag bit.

Enumerator
HRS_C_BIT_RATE_FORMAT | Heart Rate Value Format bit.
HRS_C_BIT_SENSOR_CONTACT_DETECTED | Sensor Contact Detected bit.
HRS_C_BIT_SENSOR_CONTACT_SUPPORTED | Sensor Contact Supported bit.
HRS_C_BIT_ENERGY_EXPENDED_STATUS | Energy Expended Status bit.
HRS_C_BIT_INTERVAL | RR-Interval bit.

Definition at line 95 of file hrs_c.h.

## ◆ hrs_c_sensor_loc_t

enum hrs_c_sensor_loc_t

Values for sensor location.

Enumerator
HRS_C_SENS_LOC_OTHER | The sensor location is other.
HRS_C_SENS_LOC_CHEST | The sensor location is the chest.
HRS_C_SENS_LOC_WRIST | The sensor location is the wrist.
HRS_C_SENS_LOC_FINGER | The sensor location is the finger.
HRS_C_SENS_LOC_HAND | The sensor location is the hand.
HRS_C_SENS_LOC_EARLOBE | The sensor location is the earlobe.
HRS_C_SENS_LOC_FOOT | The sensor location is the foot.

Definition at line 106 of file hrs_c.h.