Macros
Interrupt Defines
Peripheral Driver » LL Driver » I2S » Defines » I2S Exported Constants

Interrupt definitions which can be used with LL_SPI_ReadReg and LL_SPI_WriteReg functions. More...

## Macros
#define | LL_I2S_INT_TXFO I2S_INTMASK_TXFO
| TX FIFO write overflow interrupt More...
#define | LL_I2S_INT_TXFE I2S_INTMASK_TXFE
| TX FIFO threshold level is not reached interrupt. More...
#define | LL_I2S_INT_RXFO I2S_INTMASK_RXFO
| RX FIFO receive overflow interrupt More...
#define | LL_I2S_INT_RXDA I2S_INTMASK_RXDA
| RX FIFO threshold level is reached interrupt More...

## Detailed Description

Interrupt definitions which can be used with LL_SPI_ReadReg and LL_SPI_WriteReg functions.

## Macro Definition Documentation

## ◆ LL_I2S_INT_RXDA

#define LL_I2S_INT_RXDA I2S_INTMASK_RXDA

RX FIFO threshold level is reached interrupt

Definition at line 140 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_INT_RXFO

#define LL_I2S_INT_RXFO I2S_INTMASK_RXFO

RX FIFO receive overflow interrupt

Definition at line 139 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_INT_TXFE

#define LL_I2S_INT_TXFE I2S_INTMASK_TXFE

TX FIFO threshold level is not reached interrupt.

Definition at line 138 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_INT_TXFO

#define LL_I2S_INT_TXFO I2S_INTMASK_TXFO

TX FIFO write overflow interrupt

Definition at line 137 of file gr55xx_ll_i2s.h.