Data Fields
ble_escs_init_params_t Struct Reference
BLE Services » BLE Eddystone Configuration Service (ESCS)

EddyStone Configuration Service environment variable. More...

`#include <escs.h>`

## Data Fields
uint8_t | active_slot_no
uint8_t | lock_state
uint16_t | adv_interval
int8_t | slot_tx_power [APP_MAX_ADV_SLOTS]
int8_t | adv_tx_power
bool | remain_connectable
slot_lock_code_t | beacon_lock_code

## Detailed Description

EddyStone Configuration Service environment variable.

## Field Documentation

## ◆ active_slot_no

uint8_t ble_escs_init_params_t::active_slot_no

curret active slot number.

## ◆ adv_interval

uint16_t ble_escs_init_params_t::adv_interval

advertising interval.

## ◆ adv_tx_power

int8_t ble_escs_init_params_t::adv_tx_power

advertised tx Power.

## ◆ beacon_lock_code

slot_lock_code_t ble_escs_init_params_t::beacon_lock_code

beacon lock code.

## ◆ lock_state

uint8_t ble_escs_init_params_t::lock_state

beacon lock state.

## ◆ remain_connectable

bool ble_escs_init_params_t::remain_connectable

whether to remain connectable.

## ◆ slot_tx_power

int8_t ble_escs_init_params_t::slot_tx_power[APP_MAX_ADV_SLOTS]

radio tx power.

The documentation for this struct was generated from the following file:

- escs.h