### - i -

- i2c_abort_cplt_callback : _hal_i2c_callback
- i2c_error_callback : _hal_i2c_callback
- i2c_listen_cplt_callback : _hal_i2c_callback
- i2c_master_rx_cplt_callback : _hal_i2c_callback
- i2c_master_tx_cplt_callback : _hal_i2c_callback
- i2c_mem_rx_cplt_callback : _hal_i2c_callback
- i2c_mem_tx_cplt_callback : _hal_i2c_callback
- i2c_msp_deinit : _hal_i2c_callback
- i2c_msp_init : _hal_i2c_callback
- i2c_slave_rx_cplt_callback : _hal_i2c_callback
- i2c_slave_tx_cplt_callback : _hal_i2c_callback
- i2s_error_callback : _hal_i2s_callback
- i2s_msp_deinit : _hal_i2s_callback
- i2s_msp_init : _hal_i2s_callback
- i2s_rx_cplt_callback : _hal_i2s_callback
- i2s_tx_cplt_callback : _hal_i2s_callback
- i2s_tx_rx_cplt_callback : _hal_i2s_callback
- ias_alert_level_handle : ias_c_handles_t
- ias_srvc_end_handle : ias_c_handles_t
- ias_srvc_start_handle : ias_c_handles_t
- id : app_dual_tim_params_t , app_i2c_params_t , app_i2s_params_t , app_pwm_params_t , app_qspi_params_t , app_spi_params_t , app_tim_params_t , app_uart_params_t
- ikey_dist : sec_param_t
- impedance : bcs_meas_val_t
- impedance_present : bcs_meas_flag_t
- important : ancs_ntf_flags_t
- inc_srvc : gattc_browse_attr_info
- inc_srvc_handle : gatts_create_db_t
- inc_srvc_num : gatts_create_db_t
- includes : ble_gattc_incl_disc_t
- index : gap_get_bd_addr_t
- info : ble_gattc_browse_srvc_t , gap_conn_info_param_t
- info_mode : _efuse_init
- init : _adc_handle , _aes_handle , _aon_wdt_handle , _comp_handle , _dma_handle , _dual_timer_handle , _efuse_handle , _hmac_handle , _i2c_handle , _i2s_handle , _iso7816_handle_t , _pkc_handle , _qspi_handle , _rng_handle , _spi_handle , _timer_handle , _uart_handle , _wdt_handle , _xqspi_handle_t , app_adc_params_t , app_aes_params_t , app_comp_params_t , app_dma_params_t , app_dual_tim_params_t , app_hmac_params_t , app_i2c_params_t , app_i2s_params_t , app_pkc_params_t , app_pwm_params_t , app_qspi_params_t , app_rng_params_t , app_spi_params_t , app_tim_params_t , app_uart_params_t , ble_prf_manager_cbs_t , hci_uart_call_t , pwm_handle_t
- initial_alert_level : lls_init_t
- initial_tx_power_level : tps_init_t
- input : app_comp_pin_cfg_t
- input_mode : _ll_adc_init
- input_report_array : hids_init_t
- input_report_count : hids_init_t
- input_source : _ll_comp_init
- inst : _xqspi_command_t
- inst_addr_mode : _xqspi_command_t
- inst_addr_transfer_format : _ll_qspi_init_t
- inst_cadence : rscs_c_meas_val_t , rscs_meas_val_t
- inst_size : _xqspi_command_t
- inst_speed : rscs_c_meas_val_t , rscs_meas_val_t
- inst_stride_length : rscs_c_meas_val_t , rscs_meas_val_t
- inst_stride_length_present : rscs_c_meas_val_t , rscs_meas_val_t
- instruction : _qspi_command_t
- instruction_address_mode : _qspi_command_t
- instruction_size : _ll_qspi_init_t , _qspi_command_t
- interrupt : _ll_rng_init
- interval : _calendar_handle , gap_con_plan_tag_t , gap_conn_update_cmp_t , gap_scan_param_t
- interval_max : gap_conn_param_t , gap_conn_update_param_t , gap_init_param_t
- interval_min : gap_conn_param_t , gap_conn_update_param_t , gap_init_param_t
- intv : gap_sync_established_ind_t
- io_0 : app_qspi_pin_cfg_t
- io_1 : app_qspi_pin_cfg_t
- io_2 : app_qspi_pin_cfg_t
- io_3 : app_qspi_pin_cfg_t
- io_cap : sec_param_t
- io_evt_cb : app_gpiote_param_t
- io_ldo_bypass : pmu_trim_info_t
- io_ldo_vout : pmu_trim_info_t
- is_active : ags_stream_env_t
- is_dap_boot : boot_info_t
- is_enter_lp_mode : dss_evt_t
- is_inc_prama : hrrcps_rsp_val_t
- is_kb : hids_init_t
- is_last_trans : _hmac_handle
- is_mouse : hids_init_t
- is_run_or_walk : rscs_c_meas_val_t , rscs_meas_val_t
- is_sensor_contact_detected : hrs_c_hr_meas_t
- is_sensor_contact_supported : hrs_init_t
- iso7816_abort_cplt_callback : _iso7816_callback
- iso7816_atr_cplt_callback : _iso7816_callback
- iso7816_error_callback : _iso7816_callback
- iso7816_msp_deinit : _iso7816_callback
- iso7816_msp_init : _iso7816_callback
- iso7816_presence_callback : _iso7816_callback
- iso7816_rx_cplt_callback : _iso7816_callback
- iso7816_tx_cplt_callback : _iso7816_callback
- iso7816_tx_rx_cplt_callback : _iso7816_callback
- items : bond_dev_list_t , period_adv_list_t , ral_dev_list_t , white_list_t