Macros
Defines
BLE Services » Apple Notification Center Service (ANCS)

## Macros
#define | ANCS_C_CONNECTION_MAX
| Maximum number of ANCS Client connections. More...
#define | ANCS_SRVC_UUID
| UUID of Apple notification center service. More...
#define | ANCS_NTF_SOURCE_UUID
| UUID of notification source. More...
#define | ANCS_CONTROL_POINT_UUID
| UUID of control point. More...
#define | ANCS_DATA_SOURCE_UUID
| UUID of data source. More...

## Detailed Description

## Macro Definition Documentation

## ◆ ANCS_C_CONNECTION_MAX

#define ANCS_C_CONNECTION_MAX

Value:
(10 < CFG_MAX_CONNECTIONS ?\
10 : CFG_MAX_CONNECTIONS)

Maximum number of ANCS Client connections.

Definition at line 82 of file ancs_c.h.

## ◆ ANCS_CONTROL_POINT_UUID

#define ANCS_CONTROL_POINT_UUID

Value:
0xd9, 0xd9, 0xaa, 0xfd, 0xbd, 0x9b, 0x21, 0x98,\
0xa8, 0x49, 0xe1, 0x45, 0xf3, 0xd8, 0xd1, 0x69

UUID of control point.

Definition at line 88 of file ancs_c.h.

## ◆ ANCS_DATA_SOURCE_UUID

#define ANCS_DATA_SOURCE_UUID

Value:
0xfb, 0x7b, 0x7c, 0xce, 0x6a, 0xb3, 0x44, 0xbe,\
0xb5, 0x4b, 0xd6, 0x24, 0xe9, 0xc6, 0xea, 0x22

UUID of data source.

Definition at line 90 of file ancs_c.h.

## ◆ ANCS_NTF_SOURCE_UUID

#define ANCS_NTF_SOURCE_UUID

Value:
0xbd, 0x1d, 0xa2, 0x99, 0xe6, 0x25, 0x58, 0x8c,\
0xd9, 0x42, 0x01, 0x63, 0x0d, 0x12, 0xbf, 0x9f

UUID of notification source.

Definition at line 86 of file ancs_c.h.

## ◆ ANCS_SRVC_UUID

#define ANCS_SRVC_UUID

Value:
0xd0, 0x00, 0x2d, 0x12, 0x1e, 0x4b, 0x0f, 0xa4,\
0x99,0x4e, 0xce, 0xb5, 0x31, 0xf4, 0x05, 0x79

UUID of Apple notification center service.

Definition at line 84 of file ancs_c.h.