Modules | Macros
Defines
BLE Services » Wechat (WECHAT)

## Modules
| WECHAT Service and Characteristic UUID
| WeChat Service, Airsync and Pedometer Characteristic UUID.
| WECHAT pedeometer measurement flag
| WeChat pedeometer measurement flag bits.

## Macros
#define | WECHAT_CONNECTION_MAX
| Maximum number of WeChat connections. More...
#define | WECHAT_DATA_LEN 20
| Maximum length of WeChat Data. More...
#define | WECHAT_PEDO_TARGET_VAL_LEN 0x04
| Maximum length of WeChat pedometer target value. More...
#define | WECHAT_PEDO_STEP_COUNT_MAX 0xFFFFFF
| Maximum value of WeChat pedometer step count. More...

## Detailed Description

## Macro Definition Documentation

## ◆ WECHAT_CONNECTION_MAX

#define WECHAT_CONNECTION_MAX

Value:
(10 < CFG_MAX_CONNECTIONS ?\
10 : CFG_MAX_CONNECTIONS)

Maximum number of WeChat connections.

Definition at line 76 of file wechat.h.

## ◆ WECHAT_DATA_LEN

#define WECHAT_DATA_LEN 20

Maximum length of WeChat Data.

Definition at line 77 of file wechat.h.

## ◆ WECHAT_PEDO_STEP_COUNT_MAX

#define WECHAT_PEDO_STEP_COUNT_MAX 0xFFFFFF

Maximum value of WeChat pedometer step count.

Definition at line 79 of file wechat.h.

## ◆ WECHAT_PEDO_TARGET_VAL_LEN

#define WECHAT_PEDO_TARGET_VAL_LEN 0x04

Maximum length of WeChat pedometer target value.

Definition at line 78 of file wechat.h.