Classes | Macros | Typedefs | Enumerations | Functions
pcs.h File Reference

Power Consumption Service API. More...

`#include "gr55xx_sys.h"`
`#include "custom_config.h"`

Go to the source code of this file.

## Classes
struct | pcs_evt_t
| PCS Service event. More...
struct | pcs_init_t
| PCS Service init stucture. More...

## Macros
#define | PCS_CONNECTION_MAX
| Maximum number of Power Consumption Service connections. More...
#define | PCS_MAX_DATA_LEN 244
| Maximum length of application data packet which is transmitted via PCS. More...
#define | PCS_SERVICE_UUID
| The UUID of Power Consumption Service for setting advertising data. More...
#define | PCS_SET_PARAM_SUCCESS 0x00
| PCS parameters set successfully. More...
#define | PCS_SET_PARAM_FAIL 0x81
| PCS parameters set unsuccessfully. More...
#define | PCS_SET_ADV_DATA_3B 0x03
| Set 3 byte advertising data. More...
#define | PCS_SET_ADV_DATA_10B 0x0a
| Set 10 byte advertising data. More...
#define | PCS_SET_ADV_DATA_17B 0x11
| Set 17 byte advertising data. More...
#define | PCS_SET_ADV_DATA_24B 0x18
| Set 24 byte advertising data. More...
#define | PCS_SET_ADV_DATA_31B 0x1f
| Set 31 byte advertising data. More...

## Typedefs
typedef void(* | pcs_evt_handler_t) (pcs_evt_t *p_evt)
| PCS Service event handler type. More...

## Enumerations
enum | pcs_evt_type_t { PCS_EVT_INVALID, PCS_EVT_TX_ENABLE, PCS_EVT_TX_DISABLE, PCS_EVT_SETTING_ENABLE, PCS_EVT_SETTING_DISABLE, PCS_EVT_TX_DATA_SENT, PCS_EVT_PARAM_SET, PCS_EVT_DISCONNECTED }
| PCS Service event types. More...
enum | pcs_setting_type_t { PCS_SETTING_TYPE_ADV_INTERVAL, PCS_SETTING_TYPE_CONN_PARAM, PCS_SETTING_TYPE_PHY, PCS_SETTING_TYPE_ADV_DATA, PCS_SETTING_TYPE_TX_POWER }
| PCS Service settings types. More...

## Functions
sdk_err_t | pcs_service_init (pcs_init_t *p_pcs_init)
| Initialize a PCS Service instance and add in the database. More...
sdk_err_t | pcs_tx_data_send (uint8_t conn_idx, uint8_t *p_data, uint16_t length)
| Send data to peer device. More...
sdk_err_t | pcs_setting_reply (uint8_t conn_idx, uint8_t *p_data, uint16_t length)
| Reply parameters set result. More...

## Detailed Description

Power Consumption Service API.

Attention

  ##### Copyright (c) 2019 GOODIX

All rights reserved.

Redistribution and use in source and binary forms, with or without modification, are permitted provided that the following conditions are met: Redistributions of source code must retain the above copyright notice, this list of conditions and the following disclaimer. Redistributions in binary form must reproduce the above copyright notice, this list of conditions and the following disclaimer in the documentation and/or other materials provided with the distribution. Neither the name of GOODIX nor the names of its contributors may be used to endorse or promote products derived from this software without specific prior written permission.

THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL COPYRIGHT HOLDERS AND CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.

Definition in file pcs.h.