Macros
Defines
BLE Services » HRS RSCS Relay Control Point Service (HRRCPS)

## Macros
#define | HRRCPS_CONNECTION_MAX
| Maximum number of HRS RSCS Relay Control Point Service connections. More...
#define | HRRCPS_CTRL_PT_VAL_LEN 2
| Length of the value of Control Point characteristic. More...
#define | HRRCPS_CTRL_PT_RSP_VAL_LEN 4
| Length of the value of Control Point Response characteristic. More...
#define | HRRCPS_SERVICE_UUID
| The UUID of HRS RSCS Relay Control Point Service for setting advertising data. More...

## Detailed Description

## Macro Definition Documentation

## ◆ HRRCPS_CONNECTION_MAX

#define HRRCPS_CONNECTION_MAX

Value:
(10 < CFG_MAX_CONNECTIONS ?\
10 : CFG_MAX_CONNECTIONS)

Maximum number of HRS RSCS Relay Control Point Service connections.

Definition at line 71 of file hrrcps.h.

## ◆ HRRCPS_CTRL_PT_RSP_VAL_LEN

#define HRRCPS_CTRL_PT_RSP_VAL_LEN 4

Length of the value of Control Point Response characteristic.

Definition at line 73 of file hrrcps.h.

## ◆ HRRCPS_CTRL_PT_VAL_LEN

#define HRRCPS_CTRL_PT_VAL_LEN 2

Length of the value of Control Point characteristic.

Definition at line 72 of file hrrcps.h.

## ◆ HRRCPS_SERVICE_UUID

#define HRRCPS_SERVICE_UUID

Value:
0x1B, 0xD7, 0x90, 0xEC, 0xE8, 0xB9, 0x75, 0x80,\
0x0A, 0x46, 0x44, 0xD3, 0x01, 0x06, 0xED, 0xA6

The UUID of HRS RSCS Relay Control Point Service for setting advertising data.

Definition at line 75 of file hrrcps.h.