Macros
XQSPI Instruction and Address Mode, only in QSPI mode
Peripheral Driver » HAL Driver » XQSPI » Defines » XQSPI Exported Constants

## Macros
#define | XQSPI_INST_ADDR_ALL_IN_SPI (0)
| Instruction and address are sent in SPI mode. More...
#define | XQSPI_INST_IN_SPI_ADDR_IN_SPIFRF (1)
| Instruction is sent in SPI mode, and address is sent in Daul/Quad SPI mode. More...
#define | XQSPI_INST_ADDR_ALL_IN_SPIFRF (2)
| Instruction and address are sent in Daul/Quad SPI mode. More...

## Detailed Description

## Macro Definition Documentation

## ◆ XQSPI_INST_ADDR_ALL_IN_SPI

#define XQSPI_INST_ADDR_ALL_IN_SPI (0)

Instruction and address are sent in SPI mode.

Definition at line 325 of file gr55xx_hal_xqspi.h.

## ◆ XQSPI_INST_ADDR_ALL_IN_SPIFRF

#define XQSPI_INST_ADDR_ALL_IN_SPIFRF (2)

Instruction and address are sent in Daul/Quad SPI mode.

Definition at line 327 of file gr55xx_hal_xqspi.h.

## ◆ XQSPI_INST_IN_SPI_ADDR_IN_SPIFRF

#define XQSPI_INST_IN_SPI_ADDR_IN_SPIFRF (1)

Instruction is sent in SPI mode, and address is sent in Daul/Quad SPI mode.

Definition at line 326 of file gr55xx_hal_xqspi.h.