Macros
Characteristics Mask
BLE Services » Health Thermometer Service (HTS) » Defines

Bit masks for the initialization of hts_init_t::char_mask. More...

## Macros
#define | HTS_CHAR_MANDATORY 0x000f
| Bit mask for mandatory characteristic in HTS. More...
#define | HTS_CHAR_TEM_TYPE_SUP 0x003f
| Bit mask for temperature type characteristic that is optional. More...
#define | HTS_CHAR_INTM_TEM_SUP 0x01c0
| Bit mask for intermediate temperature characteristic that is optional. More...
#define | HTS_CHAR_MEAS_INTERVAL_SUP 0x1e00
| Bit mask for mearsurement interval characteristic that is optional. More...
#define | HTS_CHAR_FULL 0x1fff
| Bit mask of the full characteristic. More...

## Detailed Description

Bit masks for the initialization of hts_init_t::char_mask.

## Macro Definition Documentation

## ◆ HTS_CHAR_FULL

#define HTS_CHAR_FULL 0x1fff

Bit mask of the full characteristic.

Definition at line 92 of file hts.h.

## ◆ HTS_CHAR_INTM_TEM_SUP

#define HTS_CHAR_INTM_TEM_SUP 0x01c0

Bit mask for intermediate temperature characteristic that is optional.

Definition at line 90 of file hts.h.

## ◆ HTS_CHAR_MANDATORY

#define HTS_CHAR_MANDATORY 0x000f

Bit mask for mandatory characteristic in HTS.

Definition at line 88 of file hts.h.

## ◆ HTS_CHAR_MEAS_INTERVAL_SUP

#define HTS_CHAR_MEAS_INTERVAL_SUP 0x1e00

Bit mask for mearsurement interval characteristic that is optional.

Definition at line 91 of file hts.h.

## ◆ HTS_CHAR_TEM_TYPE_SUP

#define HTS_CHAR_TEM_TYPE_SUP 0x003f

Bit mask for temperature type characteristic that is optional.

Definition at line 89 of file hts.h.