Enumerations
Enumerations
Peripheral Driver » APP DRIVER » QSPI

## Enumerations
enum | app_qspi_id_t { APP_QSPI_ID_0, APP_QSPI_ID_1, APP_QSPI_ID_MAX }
| QSPI module Enumerations definition. More...
enum | app_qspi_type_t { APP_QSPI_TYPE_INTERRUPT, APP_QSPI_TYPE_POLLING, APP_QSPI_TYPE_DMA, APP_QSPI_TYPE_MAX }
| QSPI operating mode Enumerations definition. More...
enum | app_qspi_evt_type_t { APP_QSPI_EVT_ERROR, APP_QSPI_EVT_TX_CPLT, APP_QSPI_EVT_RX_DATA }
| APP QSPI Event Type. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ app_qspi_evt_type_t

enum app_qspi_evt_type_t

APP QSPI Event Type.

Enumerator
APP_QSPI_EVT_ERROR | Error reported by UART peripheral.
APP_QSPI_EVT_TX_CPLT | Requested TX transfer completed.
APP_QSPI_EVT_RX_DATA | Requested RX transfer completed.

Definition at line 103 of file app_qspi.h.

## ◆ app_qspi_id_t

enum app_qspi_id_t

QSPI module Enumerations definition.

Enumerator
APP_QSPI_ID_0 | QSPI module 0.
APP_QSPI_ID_1 | QSPI module 1.
APP_QSPI_ID_MAX | Only for check parameter, not used as input parameters.

Definition at line 82 of file app_qspi.h.

## ◆ app_qspi_type_t

enum app_qspi_type_t

QSPI operating mode Enumerations definition.

Enumerator
APP_QSPI_TYPE_INTERRUPT | Interrupt operation mode.
APP_QSPI_TYPE_POLLING | Polling operation mode
APP_QSPI_TYPE_DMA | DMA operation mode
APP_QSPI_TYPE_MAX | Only for check parameter, not used as input parameters.

Definition at line 92 of file app_qspi.h.