### - r -

- REMOTE_USER_TERM_CON : ble_l2cap.h
- RNG_OSC_CLK : platform_sdk.h
- RNG_OSC_CLK2 : platform_sdk.h
- RSCS_C_CTRL_PT_OP_REQ_SUP_LOC : rscs_c.h
- RSCS_C_CTRL_PT_OP_RESERVED : rscs_c.h
- RSCS_C_CTRL_PT_OP_RSP_CODE : rscs_c.h
- RSCS_C_CTRL_PT_OP_SET_CUMUL_VAL : rscs_c.h
- RSCS_C_CTRL_PT_OP_START_CALIB : rscs_c.h
- RSCS_C_CTRL_PT_OP_UPD_LOC : rscs_c.h
- RSCS_C_CTRL_PT_RSP_FAILED : rscs_c.h
- RSCS_C_CTRL_PT_RSP_INVALID_PARAM : rscs_c.h
- RSCS_C_CTRL_PT_RSP_NOT_SUP : rscs_c.h
- RSCS_C_CTRL_PT_RSP_RESERVED : rscs_c.h
- RSCS_C_CTRL_PT_RSP_SUCCESS : rscs_c.h
- RSCS_C_EVT_CTRL_PT_IND_SET_SUCCESS : rscs_c.h
- RSCS_C_EVT_CTRL_PT_RSP_RECEIVE : rscs_c.h
- RSCS_C_EVT_CTRL_PT_SET_SUCCESS : rscs_c.h
- RSCS_C_EVT_DISCOVERY_COMPLETE : rscs_c.h
- RSCS_C_EVT_DISCOVERY_FAIL : rscs_c.h
- RSCS_C_EVT_INVALID : rscs_c.h
- RSCS_C_EVT_RSC_FEATURE_RECEIVE : rscs_c.h
- RSCS_C_EVT_RSC_MEAS_NTF_SET_SUCCESS : rscs_c.h
- RSCS_C_EVT_RSC_MEAS_VAL_RECEIVE : rscs_c.h
- RSCS_C_EVT_SENSOR_LOC_RECEIVE : rscs_c.h
- RSCS_C_EVT_WRITE_OP_ERR : rscs_c.h
- RSCS_C_SENSOR_LOC_FRONT_HUB : rscs_c.h
- RSCS_C_SENSOR_LOC_FRONT_WHEEL : rscs_c.h
- RSCS_C_SENSOR_LOC_HIP : rscs_c.h
- RSCS_C_SENSOR_LOC_LEFT_PEDAL : rscs_c.h
- RSCS_C_SENSOR_LOC_OTHER : rscs_c.h
- RSCS_C_SENSOR_LOC_RIGHT_PEDAL : rscs_c.h
- RSCS_C_SENSOR_LOC_SHOE_IN : rscs_c.h
- RSCS_C_SENSOR_LOC_SHOE_TOP : rscs_c.h
- RSCS_C_SENSOR_LOC_SUP_NB : rscs_c.h
- RSCS_CTRL_PT_OP_REQ_SUP_LOC : rscs.h
- RSCS_CTRL_PT_OP_RESERVED : rscs.h
- RSCS_CTRL_PT_OP_RSP_CODE : rscs.h
- RSCS_CTRL_PT_OP_SET_CUMUL_VAL : rscs.h
- RSCS_CTRL_PT_OP_START_CALIB : rscs.h
- RSCS_CTRL_PT_OP_UPD_LOC : rscs.h
- RSCS_CTRL_PT_RSP_FAILED : rscs.h
- RSCS_CTRL_PT_RSP_INVALID_PARAM : rscs.h
- RSCS_CTRL_PT_RSP_NOT_SUP : rscs.h
- RSCS_CTRL_PT_RSP_RESERVED : rscs.h
- RSCS_CTRL_PT_RSP_SUCCESS : rscs.h
- RSCS_EVT_CTRL_POINT_INDICATION_DISABLE : rscs.h
- RSCS_EVT_CTRL_POINT_INDICATION_ENABLE : rscs.h
- RSCS_EVT_CTRL_POINT_RSP_CPLT : rscs.h
- RSCS_EVT_CUMUL_VAL_SET : rscs.h
- RSCS_EVT_INVALID : rscs.h
- RSCS_EVT_RSC_MEAS_NOTIFICATION_DISABLE : rscs.h
- RSCS_EVT_RSC_MEAS_NOTIFICATION_ENABLE : rscs.h
- RSCS_EVT_RSC_MEAS_SEND_CPLT : rscs.h
- RSCS_EVT_SEBSOR_CALIBRATION : rscs.h
- RSCS_EVT_SEBSOR_LOC_UPD : rscs.h
- RSCS_EVT_SUP_SEBSOR_LOC_REQ : rscs.h
- RSCS_SENSOR_LOC_FRONT_HUB : rscs.h
- RSCS_SENSOR_LOC_FRONT_WHEEL : rscs.h
- RSCS_SENSOR_LOC_HIP : rscs.h
- RSCS_SENSOR_LOC_LEFT_PEDAL : rscs.h
- RSCS_SENSOR_LOC_OTHER : rscs.h
- RSCS_SENSOR_LOC_RIGHT_PEDAL : rscs.h
- RSCS_SENSOR_LOC_SHOE_IN : rscs.h
- RSCS_SENSOR_LOC_SHOE_TOP : rscs.h
- RSCS_SENSOR_LOC_SUP_NB : rscs.h
- RTC_OSC_CLK : platform_sdk.h
- RTUS_CTRL_PT_CANCEL_UPDATE : rtus.h
- RTUS_CTRL_PT_GET_UPDATE : rtus.h
- RTUS_CUR_STATE_IDLE : rtus.h
- RTUS_CUR_STATE_PENDING : rtus.h
- RTUS_EVT_CANCEL_UPDATE : rtus.h
- RTUS_EVT_GET_UPDATE : rtus.h
- RTUS_EVT_INVALID : rtus.h
- RTUS_UPDATE_RESULT_CANCELED : rtus.h
- RTUS_UPDATE_RESULT_NO_ATTEMPTED : rtus.h
- RTUS_UPDATE_RESULT_NO_CONN_TO_REF : rtus.h
- RTUS_UPDATE_RESULT_REP_ERROR : rtus.h
- RTUS_UPDATE_RESULT_SCCESSFUL : rtus.h
- RTUS_UPDATE_RESULT_TIMEOUT : rtus.h