Macros
AON_GPIO mode
Peripheral Driver » HAL Driver » AON_GPIO » Defines » AON_GPIO Exported Constants

AON_GPIO Configuration Mode Elements values convention: 0x000000YX. More...

## Macros
#define | AON_GPIO_MODE_INPUT (LL_AON_GPIO_MODE_INPUT << 0)
| Input Mode More...
#define | AON_GPIO_MODE_OUTPUT (LL_AON_GPIO_MODE_OUTPUT << 0)
| Output Mode More...
#define | AON_GPIO_MODE_MUX (LL_GPIO_MODE_MUX << 0)
| Mux Mode More...
#define | AON_GPIO_MODE_IT_RISING (LL_AON_GPIO_TRIGGER_RISING << 4)
| Interrupt Mode with Rising edge trigger detection More...
#define | AON_GPIO_MODE_IT_FALLING (LL_AON_GPIO_TRIGGER_FALLING << 4)
| Interrupt Mode with Falling edge trigger detection. More...
#define | AON_GPIO_MODE_IT_HIGH (LL_AON_GPIO_TRIGGER_HIGH << 4)
| Interrupt Mode with High-level trigger detection More...
#define | AON_GPIO_MODE_IT_LOW (LL_AON_GPIO_TRIGGER_LOW << 4)
| Interrupt Mode with Low-level trigger detection More...

## Detailed Description

AON_GPIO Configuration Mode Elements values convention: 0x000000YX.

- X : IO Direction mode (Input, Output, Mux)
- Y : IT trigger detection

## Macro Definition Documentation

## ◆ AON_GPIO_MODE_INPUT

#define AON_GPIO_MODE_INPUT (LL_AON_GPIO_MODE_INPUT << 0)

Input Mode

Definition at line 157 of file gr55xx_hal_aon_gpio.h.

## ◆ AON_GPIO_MODE_IT_FALLING

#define AON_GPIO_MODE_IT_FALLING (LL_AON_GPIO_TRIGGER_FALLING << 4)

Interrupt Mode with Falling edge trigger detection.

Definition at line 161 of file gr55xx_hal_aon_gpio.h.

## ◆ AON_GPIO_MODE_IT_HIGH

#define AON_GPIO_MODE_IT_HIGH (LL_AON_GPIO_TRIGGER_HIGH << 4)

Interrupt Mode with High-level trigger detection

Definition at line 162 of file gr55xx_hal_aon_gpio.h.

## ◆ AON_GPIO_MODE_IT_LOW

#define AON_GPIO_MODE_IT_LOW (LL_AON_GPIO_TRIGGER_LOW << 4)

Interrupt Mode with Low-level trigger detection

Definition at line 163 of file gr55xx_hal_aon_gpio.h.

## ◆ AON_GPIO_MODE_IT_RISING

#define AON_GPIO_MODE_IT_RISING (LL_AON_GPIO_TRIGGER_RISING << 4)

Interrupt Mode with Rising edge trigger detection

Definition at line 160 of file gr55xx_hal_aon_gpio.h.

## ◆ AON_GPIO_MODE_MUX

#define AON_GPIO_MODE_MUX (LL_GPIO_MODE_MUX << 0)

Mux Mode

Definition at line 159 of file gr55xx_hal_aon_gpio.h.

## ◆ AON_GPIO_MODE_OUTPUT

#define AON_GPIO_MODE_OUTPUT (LL_AON_GPIO_MODE_OUTPUT << 0)

Output Mode

Definition at line 158 of file gr55xx_hal_aon_gpio.h.