Macros
CTS Pin State
Peripheral Driver » LL Driver » UART » Defines » UART Exported Constants

## Macros
#define | LL_UART_CTSPIN_STATE_ACTIVE 0x00000001U
| CTS pin active(Logic 1) More...
#define | LL_UART_CTSPIN_STATE_INACTIVE 0x00000000U
| CTS pin pin inactive(Logic 0) More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_UART_CTSPIN_STATE_ACTIVE

#define LL_UART_CTSPIN_STATE_ACTIVE 0x00000001U

CTS pin active(Logic 1)

Definition at line 214 of file gr55xx_ll_uart.h.

## ◆ LL_UART_CTSPIN_STATE_INACTIVE

#define LL_UART_CTSPIN_STATE_INACTIVE 0x00000000U

CTS pin pin inactive(Logic 0)

Definition at line 215 of file gr55xx_ll_uart.h.