Public Attributes | List of all members
gap_ext_adv_report_ind_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control » Structures

APP receives the extended advertising report indication info struct. More...

`#include <ble_gapc.h>`

## Public Attributes
uint8_t | adv_type
| Advertising type. More...
uint8_t | adv_info
| Bit field providing information about the received report. More...
gap_bdaddr_t | broadcaster_addr
| Broadcaster device address. More...
gap_bdaddr_t | direct_addr
| Target address (in case of a directed advertising report). More...
int8_t | tx_pwr
| TX power (in dBm). More...
int8_t | rssi
| RSSI (between -127 and +20 dBm). More...
uint8_t | phy_prim
| Primary PHY on which advertising report has been received. More...
uint8_t | phy_second
| Secondary PHY on which advertising report has been received. More...
uint8_t | adv_sid
| Advertising SID , valid only for periodic advertising report. More...
uint16_t | period_adv_intv
| Periodic advertising interval (in unit of 1.25ms, min is 7.5ms), valid only for periodic advertising report. More...
uint8_t | per_sync_idx
| Periodic syncronization index, valid only for periodic advertising report. More...
uint16_t | length
| Report length. More...
uint8_t | data [__ARRAY_EMPTY]
| Report. More...

## Detailed Description

APP receives the extended advertising report indication info struct.

Definition at line 318 of file ble_gapc.h.

## Member Data Documentation

## ◆ adv_info

uint8_t gap_ext_adv_report_ind_t::adv_info

Bit field providing information about the received report.

See also
  enum gap_adv_report_info_t.

Definition at line 321 of file ble_gapc.h.

## ◆ adv_sid

uint8_t gap_ext_adv_report_ind_t::adv_sid

Advertising SID , valid only for periodic advertising report.

Definition at line 328 of file ble_gapc.h.

## ◆ adv_type

uint8_t gap_ext_adv_report_ind_t::adv_type

Advertising type.

See also
  enum gap_adv_report_type_t.

Definition at line 320 of file ble_gapc.h.

## ◆ broadcaster_addr

gap_bdaddr_t gap_ext_adv_report_ind_t::broadcaster_addr

Broadcaster device address.

Definition at line 322 of file ble_gapc.h.

## ◆ data

uint8_t gap_ext_adv_report_ind_t::data[__ARRAY_EMPTY]

Report.

Definition at line 332 of file ble_gapc.h.

## ◆ direct_addr

gap_bdaddr_t gap_ext_adv_report_ind_t::direct_addr

Target address (in case of a directed advertising report).

Definition at line 323 of file ble_gapc.h.

## ◆ length

uint16_t gap_ext_adv_report_ind_t::length

Report length.

Definition at line 331 of file ble_gapc.h.

## ◆ per_sync_idx

uint8_t gap_ext_adv_report_ind_t::per_sync_idx

Periodic syncronization index, valid only for periodic advertising report.

Definition at line 330 of file ble_gapc.h.

## ◆ period_adv_intv

uint16_t gap_ext_adv_report_ind_t::period_adv_intv

Periodic advertising interval (in unit of 1.25ms, min is 7.5ms), valid only for periodic advertising report.

Definition at line 329 of file ble_gapc.h.

## ◆ phy_prim

uint8_t gap_ext_adv_report_ind_t::phy_prim

Primary PHY on which advertising report has been received.

Definition at line 326 of file ble_gapc.h.

## ◆ phy_second

uint8_t gap_ext_adv_report_ind_t::phy_second

Secondary PHY on which advertising report has been received.

Definition at line 327 of file ble_gapc.h.

## ◆ rssi

int8_t gap_ext_adv_report_ind_t::rssi

RSSI (between -127 and +20 dBm).

Definition at line 325 of file ble_gapc.h.

## ◆ tx_pwr

int8_t gap_ext_adv_report_ind_t::tx_pwr

TX power (in dBm).

Definition at line 324 of file ble_gapc.h.

The documentation for this struct was generated from the following file:

- ble_gapc.h