Macros
EXFLASH Size Information
Peripheral Driver » HAL Driver » EXFLASH » Defines » EXFLASH Exported Constants

## Macros
#define | EXFLASH_SIZE_PAGE_BYTES ((uint32_t)256)
| Page size in Bytes More...
#define | EXFLASH_SIZE_SECTOR_BYTES ((uint32_t)4096)
| Sector size in Bytes More...
#define | EXFLASH_SIZE_CHIP_BYTES ((uint32_t)0x800000)
| Chip size in Bytes More...
#define | EXFLASH_START_ADDR FLASH_BASE
| Flash start address More...
#define | EXFLASH_SIZE (0x00800000UL)
| Flash size More...
#define | EXFLASH_END_ADDR (EXFLASH_START_ADDR + EXFLASH_SIZE)
| Flash end address More...
#define | EXFLASH_ALIAS_OFFSET (0x02000000UL)
| Alias address offset More...
#define | EXFLASH_ALIAS_ADDR (EXFLASH_START_ADDR + EXFLASH_ALIAS_OFFSET)
| Alias start address More...

## Detailed Description

## Macro Definition Documentation

## ◆ EXFLASH_ALIAS_ADDR

#define EXFLASH_ALIAS_ADDR (EXFLASH_START_ADDR + EXFLASH_ALIAS_OFFSET)

Alias start address

Definition at line 200 of file gr55xx_hal_exflash.h.

## ◆ EXFLASH_ALIAS_OFFSET

#define EXFLASH_ALIAS_OFFSET (0x02000000UL)

Alias address offset

Definition at line 199 of file gr55xx_hal_exflash.h.

## ◆ EXFLASH_END_ADDR

#define EXFLASH_END_ADDR (EXFLASH_START_ADDR + EXFLASH_SIZE)

Flash end address

Definition at line 198 of file gr55xx_hal_exflash.h.

## ◆ EXFLASH_SIZE

#define EXFLASH_SIZE (0x00800000UL)

Flash size

Definition at line 197 of file gr55xx_hal_exflash.h.

## ◆ EXFLASH_SIZE_CHIP_BYTES

#define EXFLASH_SIZE_CHIP_BYTES ((uint32_t)0x800000)

Chip size in Bytes

Definition at line 195 of file gr55xx_hal_exflash.h.

## ◆ EXFLASH_SIZE_PAGE_BYTES

#define EXFLASH_SIZE_PAGE_BYTES ((uint32_t)256)

Page size in Bytes

Definition at line 193 of file gr55xx_hal_exflash.h.

## ◆ EXFLASH_SIZE_SECTOR_BYTES

#define EXFLASH_SIZE_SECTOR_BYTES ((uint32_t)4096)

Sector size in Bytes

Definition at line 194 of file gr55xx_hal_exflash.h.

## ◆ EXFLASH_START_ADDR

#define EXFLASH_START_ADDR FLASH_BASE

Flash start address

Definition at line 196 of file gr55xx_hal_exflash.h.