Classes | Macros | Typedefs | Enumerations | Functions
hts.h File Reference

Health Thermometer Service API. More...

`#include "gr55xx_sys.h"`
`#include "custom_config.h"`
`#include "ble_prf_utils.h"`
`#include <stdint.h>`
`#include <stdbool.h>`

Go to the source code of this file.

## Classes
struct | hts_evt_t
| Health Thermometer Service event. More...
struct | ieee_float32_t
| SFLOAT format (IEEE-11073 32-bit FLOAT, defined as a 32-bit vlue with 24-bit mantissa and 8-bit exponent. More...
struct | hts_meas_val_t
| Health Theromometer Measurement Character value structure. More...
struct | hts_init_t
| Health Thermometer Service init stucture. More...

## Macros
#define | HTS_CONNECTION_MAX
| Maximum number of Health Thermometer Service connections. More...
#define | HTS_TEM_MEAS_MAX_LEN 20
| Maximum length of temperature measurement encode. More...
#define | HTS_TEM_TYPE_MAX_LEN 1
| Maximum length of temperature type value. More...
#define | HTS_INTM_TEM_MAX_LEN 20
| Maximun length of intermediate temperature encode. More...
#define | HTS_MEAS_INTERVAL_MAX_LEN 2
| Maximum length of measurement interval value. More...
#define | HTS_MEAS_INTV_DFLT_MIN 2
| Minimun interval of temperature measurement (in unit of 1s). More...
#define | HTS_MEAS_INTV_DFLT_MAX 10
| Maximum interval of temperature measurement (in unit of 1s). More...
#define | HTS_CHAR_MANDATORY 0x000f
| Bit mask for mandatory characteristic in HTS. More...
#define | HTS_CHAR_TEM_TYPE_SUP 0x003f
| Bit mask for temperature type characteristic that is optional. More...
#define | HTS_CHAR_INTM_TEM_SUP 0x01c0
| Bit mask for intermediate temperature characteristic that is optional. More...
#define | HTS_CHAR_MEAS_INTERVAL_SUP 0x1e00
| Bit mask for mearsurement interval characteristic that is optional. More...
#define | HTS_CHAR_FULL 0x1fff
| Bit mask of the full characteristic. More...

## Typedefs
typedef void(* | hts_evt_handler_t) (hts_evt_t *p_evt)
| Health Thermometer Service event handler type. More...
typedef prf_date_time_t | hts_date_time_t
| Health Thermometer Service date time type. More...

## Enumerations
enum | hts_evt_type_t { HTS_EVT_INVALID, HTS_EVT_TEM_MEAS_INDICATION_ENABLE, HTS_EVT_TEM_MEAS_INDICATION_DISABLE, HTS_EVT_INTM_TEM_NOTIFICATION_ENABLE, HTS_EVT_INTM_TEM_NOTIFICATION_DISABLE, HTS_EVT_MEAS_INTREVAL_INDICATION_ENABLE, HTS_EVT_MEAS_INTERVAL_INDICATION_DISABLE, HTS_EVT_MEAS_INTERVAL_UPDATE, HTS_EVT_READ_CHARACTERISTIC }
| Health Thermometer Service event type. More...
enum | hts_temp_unit_t { HTS_TEMPERATURE_CELCIUS, HTS_TEMPERATURE_FAHRENHEIT }
| Health Thermometer temperature unit,. More...
enum | hts_temp_meas_type_t { HTS_TEMPERATURE_STABLE, HTS_TEMPERATURE_INTERMEDIATE }
| Health Thermometer temperature measurement type. More...
enum | hts_flag_bit_t { HTS_MEAS_FLAG_TEM_UINTS_BIT = (0x01<<0), HTS_MEAS_FLAG_TIME_STAMP_BIT = (0x01<<1), HTS_MEAS_FLAG_TEM_TYPE_BIT = (0x01<<2) }
| Health Thermometer Measurement flag bits. More...
enum | hts_temp_meas_loc_t { HTS_TEMP_TYPE_ARMPIT = 0x01, HTS_TEMP_TYPE_BODY, HTS_TEMP_TYPE_EAR, HTS_TEMP_TYPE_FINGER, HTS_TEMP_TYPE_GI_TRACT, HTS_TEMP_TYPE_MOUTH, HTS_TEMP_TYPE_RECTUM, HTS_TEMP_TYPE_TOE, HTS_TEMP_TYPE_EAR_DRUM }
| Temperature Type measurement locations. More...
enum | hts_read_characteristic_t { HTS_READ_CHAR_TEMP_TYPE, HTS_READ_CHAR_MEAS_INTL }
| The parameters for HTS_EVT_READ_CHARACTERISTIC. More...

## Functions
sdk_err_t | hts_service_init (hts_init_t *p_hts_init)
| Initialize a Health Thermometer Service instance and add in the DB. More...
sdk_err_t | hts_measurement_send (uint8_t conn_idx, hts_meas_val_t *p_meas)
| Send temperature measurement if indication or notification has been enabled. More...
sdk_err_t | hts_measurement_interval_send (uint8_t conn_idx)
| Send temperature measurement interval if indication has been enabled. More...

## Detailed Description

Health Thermometer Service API.

Attention

  ##### Copyright (c) 2019 GOODIX

All rights reserved.

Redistribution and use in source and binary forms, with or without modification, are permitted provided that the following conditions are met: Redistributions of source code must retain the above copyright notice, this list of conditions and the following disclaimer. Redistributions in binary form must reproduce the above copyright notice, this list of conditions and the following disclaimer in the documentation and/or other materials provided with the distribution. Neither the name of GOODIX nor the names of its contributors may be used to endorse or promote products derived from this software without specific prior written permission.

THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL COPYRIGHT HOLDERS AND CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.

Definition in file hts.h.