Macros
Get Flags Defines
Peripheral Driver » LL Driver » I2S » Defines » I2S Exported Constants

Flags definitions which can be used with LL_I2S_ReadReg function. More...

## Macros
#define | LL_I2S_STATUS_TXFO I2S_INTSTAT_TXFO
| TX FIFO write overflow flag More...
#define | LL_I2S_STATUS_TXFE I2S_INTSTAT_TXFE
| TX FIFO threshold level is not reached flag. More...
#define | LL_I2S_STATUS_RXFO I2S_INTSTAT_RXFO
| RX FIFO receive overflow flag More...
#define | LL_I2S_STATUS_RXDA I2S_INTSTAT_RXDA
| RX FIFO threshold level is reached flag More...

## Detailed Description

Flags definitions which can be used with LL_I2S_ReadReg function.

## Macro Definition Documentation

## ◆ LL_I2S_STATUS_RXDA

#define LL_I2S_STATUS_RXDA I2S_INTSTAT_RXDA

RX FIFO threshold level is reached flag

Definition at line 130 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_STATUS_RXFO

#define LL_I2S_STATUS_RXFO I2S_INTSTAT_RXFO

RX FIFO receive overflow flag

Definition at line 129 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_STATUS_TXFE

#define LL_I2S_STATUS_TXFE I2S_INTSTAT_TXFE

TX FIFO threshold level is not reached flag.

Definition at line 128 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_STATUS_TXFO

#define LL_I2S_STATUS_TXFO I2S_INTSTAT_TXFO

TX FIFO write overflow flag

Definition at line 127 of file gr55xx_ll_i2s.h.