Macros
GAP ADV CHANNEL (bitmask)
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Management » Defines

## Macros
#define | GAP_ADV_CHANNEL_37 0x01
| Advertising Channel 37 (2402MHz). More...
#define | GAP_ADV_CHANNEL_38 0x02
| Advertising Channel 38 (2426MHz). More...
#define | GAP_ADV_CHANNEL_39 0x04
| Advertising Channel 39 (2480MHz). More...
#define | GAP_ADV_CHANNEL_37_38_39 0x07
| Advertising Channel 37, 38, 39. More...

## Detailed Description

## Macro Definition Documentation

## ◆ GAP_ADV_CHANNEL_37

#define GAP_ADV_CHANNEL_37 0x01

Advertising Channel 37 (2402MHz).

Definition at line 145 of file ble_gapm.h.

## ◆ GAP_ADV_CHANNEL_37_38_39

#define GAP_ADV_CHANNEL_37_38_39 0x07

Advertising Channel 37, 38, 39.

Definition at line 148 of file ble_gapm.h.

## ◆ GAP_ADV_CHANNEL_38

#define GAP_ADV_CHANNEL_38 0x02

Advertising Channel 38 (2426MHz).

Definition at line 146 of file ble_gapm.h.

## ◆ GAP_ADV_CHANNEL_39

#define GAP_ADV_CHANNEL_39 0x04

Advertising Channel 39 (2480MHz).

Definition at line 147 of file ble_gapm.h.