Macros
Defines
BLE Services » Throughput Service (THS)

## Macros
#define | THS_CONNECTION_MAX
| Maximum number of Throughput Service connections. More...
#define | THS_MAX_DATA_LEN 512
| Maximum length of the value of Rx or Tx characteristic. More...
#define | THS_SERVICE_UUID
| The UUID of Throughput Service for setting advertising data. More...

## Detailed Description

## Macro Definition Documentation

## ◆ THS_CONNECTION_MAX

#define THS_CONNECTION_MAX

Value:
(10 < CFG_MAX_CONNECTIONS ?\
10 : CFG_MAX_CONNECTIONS)

Maximum number of Throughput Service connections.

Definition at line 73 of file ths.h.

## ◆ THS_MAX_DATA_LEN

#define THS_MAX_DATA_LEN 512

Maximum length of the value of Rx or Tx characteristic.

Definition at line 74 of file ths.h.

## ◆ THS_SERVICE_UUID

#define THS_SERVICE_UUID

Value:
0x1B, 0xD7, 0x90, 0xEC, 0xE8, 0xB9, 0x75, 0x80,\
0x0A, 0x46, 0x44, 0xD3, 0x01, 0x03, 0xED, 0xA6

The UUID of Throughput Service for setting advertising data.

Definition at line 76 of file ths.h.