Macros
Clock Phase
Peripheral Driver » LL Driver » SPI » Defines » SPI Exported Constants

## Macros
#define | LL_SSI_SCPHA_1EDGE 0x00000000UL
| First clock transition is the first data capture edge More...
#define | LL_SSI_SCPHA_2EDGE (1UL << SSI_CTRL0_SCPHA_Pos)
| Second clock transition is the first data capture edge. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_SSI_SCPHA_1EDGE

#define LL_SSI_SCPHA_1EDGE 0x00000000UL

First clock transition is the first data capture edge

Definition at line 329 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_SCPHA_2EDGE

#define LL_SSI_SCPHA_2EDGE (1UL << SSI_CTRL0_SCPHA_Pos)

Second clock transition is the first data capture edge.

Definition at line 330 of file gr55xx_ll_spi.h.