Macros
GAP PHYs (bitmask)
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Management » Defines

## Macros
#define | BLE_GAP_PHY_ANY 0x00
| No preferred PHY. More...
#define | BLE_GAP_PHY_LE_1MBPS (1 << 0)
| LE 1M PHY preferred for an active link. More...
#define | BLE_GAP_PHY_LE_2MBPS (1 << 1)
| LE 2M PHY preferred for an active link. More...
#define | BLE_GAP_PHY_LE_CODED (1 << 2)
| LE Coded PHY preferred for an active link. More...

## Detailed Description

## Macro Definition Documentation

## ◆ BLE_GAP_PHY_ANY

#define BLE_GAP_PHY_ANY 0x00

No preferred PHY.

Definition at line 136 of file ble_gapm.h.

## ◆ BLE_GAP_PHY_LE_1MBPS

#define BLE_GAP_PHY_LE_1MBPS (1 << 0)

LE 1M PHY preferred for an active link.

Definition at line 137 of file ble_gapm.h.

## ◆ BLE_GAP_PHY_LE_2MBPS

#define BLE_GAP_PHY_LE_2MBPS (1 << 1)

LE 2M PHY preferred for an active link.

Definition at line 138 of file ble_gapm.h.

## ◆ BLE_GAP_PHY_LE_CODED

#define BLE_GAP_PHY_LE_CODED (1 << 2)

LE Coded PHY preferred for an active link.

Definition at line 139 of file ble_gapm.h.