Macros
SCLK Gate
Peripheral Driver » LL Driver » I2S » Defines » I2S Exported Constants

## Macros
#define | LL_I2S_SCLKG_NONE (0x00000000UL)
| Clock gating is disabled. More...
#define | LL_I2S_SCLKG_CYCLES_12 (0x1UL << I2S_CLKCONFIG_SCLKG_Pos)
| Gating after 12 sclk cycles. More...
#define | LL_I2S_SCLKG_CYCLES_16 (0x2UL << I2S_CLKCONFIG_SCLKG_Pos)
| Gating after 16 sclk cycles. More...
#define | LL_I2S_SCLKG_CYCLES_20 (0x3UL << I2S_CLKCONFIG_SCLKG_Pos)
| Gating after 20 sclk cycles. More...
#define | LL_I2S_SCLKG_CYCLES_24 (0x4UL << I2S_CLKCONFIG_SCLKG_Pos)
| Gating after 24 sclk cycles. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_I2S_SCLKG_CYCLES_12

#define LL_I2S_SCLKG_CYCLES_12 (0x1UL << I2S_CLKCONFIG_SCLKG_Pos)

Gating after 12 sclk cycles.

Definition at line 202 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_SCLKG_CYCLES_16

#define LL_I2S_SCLKG_CYCLES_16 (0x2UL << I2S_CLKCONFIG_SCLKG_Pos)

Gating after 16 sclk cycles.

Definition at line 203 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_SCLKG_CYCLES_20

#define LL_I2S_SCLKG_CYCLES_20 (0x3UL << I2S_CLKCONFIG_SCLKG_Pos)

Gating after 20 sclk cycles.

Definition at line 204 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_SCLKG_CYCLES_24

#define LL_I2S_SCLKG_CYCLES_24 (0x4UL << I2S_CLKCONFIG_SCLKG_Pos)

Gating after 24 sclk cycles.

Definition at line 205 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_SCLKG_NONE

#define LL_I2S_SCLKG_NONE (0x00000000UL)

Clock gating is disabled.

Definition at line 201 of file gr55xx_ll_i2s.h.