Public Attributes | List of all members
cscs_init_t Struct Reference
BLE Services » Cycling Speed and Cadence Service (CSCS) » Structures

Cycling Speed and Cadence Service init stucture. More...

`#include <cscs.h>`

## Public Attributes
cscs_evt_handler_t | evt_handler
| Cycling Speed and Cadence Service event handler. More...
uint16_t | char_mask
| Initial mask of supported characteristics, and configured with Characteristics Mask. More...
cscs_sensor_loc_t | sensor_location
| Initial sensor location. More...
uint16_t | feature
| Initial value for features. More...

## Detailed Description

Cycling Speed and Cadence Service init stucture.

This contains all option and data needed for initialization of the service.

Definition at line 207 of file cscs.h.

## Member Data Documentation

## ◆ char_mask

uint16_t cscs_init_t::char_mask

Initial mask of supported characteristics, and configured with Characteristics Mask.

Definition at line 210 of file cscs.h.

## ◆ evt_handler

cscs_evt_handler_t cscs_init_t::evt_handler

Cycling Speed and Cadence Service event handler.

Definition at line 209 of file cscs.h.

## ◆ feature

uint16_t cscs_init_t::feature

Initial value for features.

Definition at line 212 of file cscs.h.

## ◆ sensor_location

cscs_sensor_loc_t cscs_init_t::sensor_location

Initial sensor location.

Definition at line 211 of file cscs.h.

The documentation for this struct was generated from the following file:

- cscs.h