Enumerations
Enumerations
BLE Services » Immediate Alarm Service (IAS)

## Enumerations
enum | { AMS_PLAYER_ATTR_ID_NAME, AMS_PLAYER_ATTR_ID_PLAYBACK_INFO, AMS_PLAYER_ATTR_ID_VOLUME, IAS_ALERT_NONE, IAS_ALERT_MILD, IAS_ALERT_HIGH, TRC_PWR_WFE_MODE = 0, TRC_PWR_DSLEEP_MODE, TRC_PWR_ACTIVE_MODE, TRC_PWR_BLE_RET_DSLEEP, TRC_PWR_APP_TIMER_REFUSE, TRC_PWR_APP_TIMER_PASS, TRC_PWR_BLE_TIMER_PASS }
| Immediate Alert Service Alert levels. More...
enum | ias_evt_type_t { IAS_EVT_INVALID, IAS_EVT_ALERT_LEVEL_UPDATED }
| Immediate Alert Service event type. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ anonymous enum

anonymous enum

Immediate Alert Service Alert levels.

Enumerator
AMS_PLAYER_ATTR_ID_NAME | Player attribute index of name.
AMS_PLAYER_ATTR_ID_PLAYBACK_INFO | Player attribute index of playback information.
AMS_PLAYER_ATTR_ID_VOLUME | Player attribute index of volume.
IAS_ALERT_NONE | No alert.
IAS_ALERT_MILD | Mild alert.
IAS_ALERT_HIGH | High alert.
TRC_PWR_WFE_MODE | WFE mode.
TRC_PWR_DSLEEP_MODE | Deep sleep mode.
TRC_PWR_ACTIVE_MODE | Active mode.
TRC_PWR_BLE_RET_DSLEEP | BLE return deep sleep.
TRC_PWR_APP_TIMER_REFUSE | App timer refuse.
TRC_PWR_APP_TIMER_PASS | App timer pass.
TRC_PWR_BLE_TIMER_PASS | BLE timer pass.

Definition at line 75 of file ias.h.

## ◆ ias_evt_type_t

enum ias_evt_type_t

Immediate Alert Service event type.

Enumerator
IAS_EVT_INVALID | Invalid IAS event.
IAS_EVT_ALERT_LEVEL_UPDATED | Alert Level Updated event.

Definition at line 83 of file ias.h.