Functions
Peripheral State, Mode and Error functions
Peripheral Driver » HAL Driver » I2C » Functions

Peripheral State, Mode and Error functions. More...

## Functions
hal_i2c_state_t | hal_i2c_get_state (i2c_handle_t *p_i2c)
| Return the I2C handle state. More...
hal_i2c_mode_t | hal_i2c_get_mode (i2c_handle_t *p_i2c)
| Returns the I2C Master, Slave, Memory or no mode. More...
uint32_t | hal_i2c_get_error (i2c_handle_t *p_i2c)
| Return the I2C error code. More...
hal_status_t | hal_i2c_suspend_reg (i2c_handle_t *p_i2c)
| Suspend some registers related to I2C configuration before sleep. More...
hal_status_t | hal_i2c_resume_reg (i2c_handle_t *p_i2c)
| Restore some registers related to I2C configuration after sleep. More...

## Detailed Description

Peripheral State, Mode and Error functions.

     ===============================================================================
                ##### Peripheral State, Mode and Error functions #####
     ===============================================================================
        [..]
        This subsection permit to get in run-time the status of the peripheral
        and the data flow.

## Function Documentation

## ◆ hal_i2c_get_error()

uint32_t hal_i2c_get_error | ( | i2c_handle_t * | p_i2c | ) |

Return the I2C error code.

Parameters

  [in] | p_i2c | Pointer to an I2C handle which contains the configuration information for the specified I2C.

Returns
  I2C Error Code

## ◆ hal_i2c_get_mode()

hal_i2c_mode_t hal_i2c_get_mode | ( | i2c_handle_t * | p_i2c | ) |

Returns the I2C Master, Slave, Memory or no mode.

Parameters

  [in] | p_i2c | Pointer to an I2C handle which contains the configuration information for the specified I2C.

Return values

  HAL_I2C_MODE_NONE | No I2C communication on going.
  HAL_I2C_MODE_MASTER | I2C communication is in Master Mode.
  HAL_I2C_MODE_SLAVE | I2C communication is in Slave Mode.
  HAL_I2C_MODE_MEM | I2C communication is in Memory Mode.

## ◆ hal_i2c_get_state()

hal_i2c_state_t hal_i2c_get_state | ( | i2c_handle_t * | p_i2c | ) |

Return the I2C handle state.

Parameters

  [in] | p_i2c | Pointer to an I2C handle which contains the configuration information for the specified I2C.

Return values

  HAL_I2C_STATE_RESET | Peripheral is not yet Initialized.
  HAL_I2C_STATE_READY | Peripheral Initialized and ready for use.
  HAL_I2C_STATE_BUSY | An internal process is ongoing.
  HAL_I2C_STATE_BUSY_TX | Data Transmission process is ongoing.
  HAL_I2C_STATE_BUSY_RX | Data Reception process is ongoing.
  HAL_I2C_STATE_LISTEN | Address Listen Mode is ongoing.
  HAL_I2C_STATE_BUSY_TX_LISTEN | Address Listen Mode and Data Transmission process is ongoing.
  HAL_I2C_STATE_BUSY_RX_LISTEN | Address Listen Mode and Data Reception process is ongoing.
  HAL_I2C_STATE_ABORT | Abort user request ongoing.
  HAL_I2C_STATE_TIMEOUT | Timeout state.
  HAL_I2C_STATE_ERROR | Error.

## ◆ hal_i2c_resume_reg()

hal_status_t hal_i2c_resume_reg | ( | i2c_handle_t * | p_i2c | ) |

Restore some registers related to I2C configuration after sleep.

This function must be used in conjunction with the hal_i2c_suspend_reg().

Parameters

  [in] | p_i2c | Pointer to a I2C handle which contains the configuration information for the specified I2C module.

Return values

  HAL_OK | Operation is OK.
  HAL_ERROR | Parameter error or operation not supported.
  HAL_BUSY | Driver is busy.
  HAL_TIMEOUT | Timeout occurred.

## ◆ hal_i2c_suspend_reg()

hal_status_t hal_i2c_suspend_reg | ( | i2c_handle_t * | p_i2c | ) |

Suspend some registers related to I2C configuration before sleep.

Parameters

  [in] | p_i2c | Pointer to a I2C handle which contains the configuration information for the specified I2C module.

Return values

  HAL_OK | Operation is OK.
  HAL_ERROR | Parameter error or operation not supported.
  HAL_BUSY | Driver is busy.
  HAL_TIMEOUT | Timeout occurred.