Macros
XQSPI Address Size, only in QSPI mode
Peripheral Driver » HAL Driver » XQSPI » Defines » XQSPI Exported Constants

## Macros
#define | XQSPI_ADDRSIZE_00_BITS (0)
| 0-bit (No Address) More...
#define | XQSPI_ADDRSIZE_08_BITS (1)
| 8-bit Address More...
#define | XQSPI_ADDRSIZE_16_BITS (2)
| 16-bit Address More...
#define | XQSPI_ADDRSIZE_24_BITS (3)
| 24-bit Address More...
#define | XQSPI_ADDRSIZE_32_BITS (4)
| 32-bit Address More...

## Detailed Description

## Macro Definition Documentation

## ◆ XQSPI_ADDRSIZE_00_BITS

#define XQSPI_ADDRSIZE_00_BITS (0)

0-bit (No Address)

Definition at line 315 of file gr55xx_hal_xqspi.h.

## ◆ XQSPI_ADDRSIZE_08_BITS

#define XQSPI_ADDRSIZE_08_BITS (1)

8-bit Address

Definition at line 316 of file gr55xx_hal_xqspi.h.

## ◆ XQSPI_ADDRSIZE_16_BITS

#define XQSPI_ADDRSIZE_16_BITS (2)

16-bit Address

Definition at line 317 of file gr55xx_hal_xqspi.h.

## ◆ XQSPI_ADDRSIZE_24_BITS

#define XQSPI_ADDRSIZE_24_BITS (3)

24-bit Address

Definition at line 318 of file gr55xx_hal_xqspi.h.

## ◆ XQSPI_ADDRSIZE_32_BITS

#define XQSPI_ADDRSIZE_32_BITS (4)

32-bit Address

Definition at line 319 of file gr55xx_hal_xqspi.h.