Macros
MicroWire CommandSize
Peripheral Driver » LL Driver » SPI » Defines » SPI Exported Constants

## Macros
#define | LL_SSI_MW_CMDSIZE_1BIT 0x00000000UL
| CMD length for Microwire transfer: 1 bits. More...
#define | LL_SSI_MW_CMDSIZE_2BIT (1UL << SSI_CTRL0_CFS_Pos)
| CMD length for Microwire transfer: 2 bits. More...
#define | LL_SSI_MW_CMDSIZE_3BIT (2UL << SSI_CTRL0_CFS_Pos)
| CMD length for Microwire transfer: 3 bits. More...
#define | LL_SSI_MW_CMDSIZE_4BIT (3UL << SSI_CTRL0_CFS_Pos)
| CMD length for Microwire transfer: 4 bits. More...
#define | LL_SSI_MW_CMDSIZE_5BIT (4UL << SSI_CTRL0_CFS_Pos)
| CMD length for Microwire transfer: 5 bits. More...
#define | LL_SSI_MW_CMDSIZE_6BIT (5UL << SSI_CTRL0_CFS_Pos)
| CMD length for Microwire transfer: 6 bits. More...
#define | LL_SSI_MW_CMDSIZE_7BIT (6UL << SSI_CTRL0_CFS_Pos)
| CMD length for Microwire transfer: 7 bits. More...
#define | LL_SSI_MW_CMDSIZE_8BIT (7UL << SSI_CTRL0_CFS_Pos)
| CMD length for Microwire transfer: 8 bits. More...
#define | LL_SSI_MW_CMDSIZE_9BIT (8UL << SSI_CTRL0_CFS_Pos)
| CMD length for Microwire transfer: 9 bits. More...
#define | LL_SSI_MW_CMDSIZE_10BIT (9UL << SSI_CTRL0_CFS_Pos)
| CMD length for Microwire transfer: 10 bits. More...
#define | LL_SSI_MW_CMDSIZE_11BIT (10UL << SSI_CTRL0_CFS_Pos)
| CMD length for Microwire transfer: 11 bits. More...
#define | LL_SSI_MW_CMDSIZE_12BIT (11UL << SSI_CTRL0_CFS_Pos)
| CMD length for Microwire transfer: 12 bits. More...
#define | LL_SSI_MW_CMDSIZE_13BIT (12UL << SSI_CTRL0_CFS_Pos)
| CMD length for Microwire transfer: 13 bits. More...
#define | LL_SSI_MW_CMDSIZE_14BIT (13UL << SSI_CTRL0_CFS_Pos)
| CMD length for Microwire transfer: 14 bits. More...
#define | LL_SSI_MW_CMDSIZE_15BIT (14UL << SSI_CTRL0_CFS_Pos)
| CMD length for Microwire transfer: 15 bits. More...
#define | LL_SSI_MW_CMDSIZE_16BIT (15UL << SSI_CTRL0_CFS_Pos)
| CMD length for Microwire transfer: 16 bits. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_SSI_MW_CMDSIZE_10BIT

#define LL_SSI_MW_CMDSIZE_10BIT (9UL << SSI_CTRL0_CFS_Pos)

CMD length for Microwire transfer: 10 bits.

Definition at line 294 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_MW_CMDSIZE_11BIT

#define LL_SSI_MW_CMDSIZE_11BIT (10UL << SSI_CTRL0_CFS_Pos)

CMD length for Microwire transfer: 11 bits.

Definition at line 295 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_MW_CMDSIZE_12BIT

#define LL_SSI_MW_CMDSIZE_12BIT (11UL << SSI_CTRL0_CFS_Pos)

CMD length for Microwire transfer: 12 bits.

Definition at line 296 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_MW_CMDSIZE_13BIT

#define LL_SSI_MW_CMDSIZE_13BIT (12UL << SSI_CTRL0_CFS_Pos)

CMD length for Microwire transfer: 13 bits.

Definition at line 297 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_MW_CMDSIZE_14BIT

#define LL_SSI_MW_CMDSIZE_14BIT (13UL << SSI_CTRL0_CFS_Pos)

CMD length for Microwire transfer: 14 bits.

Definition at line 298 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_MW_CMDSIZE_15BIT

#define LL_SSI_MW_CMDSIZE_15BIT (14UL << SSI_CTRL0_CFS_Pos)

CMD length for Microwire transfer: 15 bits.

Definition at line 299 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_MW_CMDSIZE_16BIT

#define LL_SSI_MW_CMDSIZE_16BIT (15UL << SSI_CTRL0_CFS_Pos)

CMD length for Microwire transfer: 16 bits.

Definition at line 300 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_MW_CMDSIZE_1BIT

#define LL_SSI_MW_CMDSIZE_1BIT 0x00000000UL

CMD length for Microwire transfer: 1 bits.

Definition at line 285 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_MW_CMDSIZE_2BIT

#define LL_SSI_MW_CMDSIZE_2BIT (1UL << SSI_CTRL0_CFS_Pos)

CMD length for Microwire transfer: 2 bits.

Definition at line 286 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_MW_CMDSIZE_3BIT

#define LL_SSI_MW_CMDSIZE_3BIT (2UL << SSI_CTRL0_CFS_Pos)

CMD length for Microwire transfer: 3 bits.

Definition at line 287 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_MW_CMDSIZE_4BIT

#define LL_SSI_MW_CMDSIZE_4BIT (3UL << SSI_CTRL0_CFS_Pos)

CMD length for Microwire transfer: 4 bits.

Definition at line 288 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_MW_CMDSIZE_5BIT

#define LL_SSI_MW_CMDSIZE_5BIT (4UL << SSI_CTRL0_CFS_Pos)

CMD length for Microwire transfer: 5 bits.

Definition at line 289 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_MW_CMDSIZE_6BIT

#define LL_SSI_MW_CMDSIZE_6BIT (5UL << SSI_CTRL0_CFS_Pos)

CMD length for Microwire transfer: 6 bits.

Definition at line 290 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_MW_CMDSIZE_7BIT

#define LL_SSI_MW_CMDSIZE_7BIT (6UL << SSI_CTRL0_CFS_Pos)

CMD length for Microwire transfer: 7 bits.

Definition at line 291 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_MW_CMDSIZE_8BIT

#define LL_SSI_MW_CMDSIZE_8BIT (7UL << SSI_CTRL0_CFS_Pos)

CMD length for Microwire transfer: 8 bits.

Definition at line 292 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_MW_CMDSIZE_9BIT

#define LL_SSI_MW_CMDSIZE_9BIT (8UL << SSI_CTRL0_CFS_Pos)

CMD length for Microwire transfer: 9 bits.

Definition at line 293 of file gr55xx_ll_spi.h.