Public Attributes | List of all members
ieee_float16_t Struct Reference
BLE Services » Blood Pressure Service (BPS) » Structures | BLE Services » Glucose Service (GLS) » Structures

SFLOAT format (IEEE-11073 16-bit FLOAT, defined as a 16-bit value with 12-bit mantissa and 4-bit exponent. More...

`#include <bps.h>`

## Public Attributes
int8_t | exponent
| Base 10 exponent, only 4 bits. More...
int16_t | mantissa
| Mantissa, only 12 bits. More...

## Detailed Description

SFLOAT format (IEEE-11073 16-bit FLOAT, defined as a 16-bit value with 12-bit mantissa and 4-bit exponent.

SFLOAT format (IEEE-11073 16-bit FLOAT, defined as a 16-bit value with 12-bit mantissa and 4-bit exponent).

Definition at line 138 of file bps.h.

## Member Data Documentation

## ◆ exponent

int8_t ieee_float16_t::exponent

Base 10 exponent, only 4 bits.

Definition at line 140 of file bps.h.

## ◆ mantissa

int16_t ieee_float16_t::mantissa

Mantissa, only 12 bits.

Definition at line 141 of file bps.h.

The documentation for this struct was generated from the following files:

- bps.h
- gls.h