Public Attributes | List of all members
gap_sync_established_ind_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control » Structures

Sync established indication. More...

`#include <ble_gapc.h>`

## Public Attributes
uint8_t | phy
| PHY on which synchronization has been established. More...
uint16_t | intv
| Periodic advertising interval (in unit of 1.25ms, min is 7.5ms). More...
uint8_t | adv_sid
| Advertising SID. More...
uint8_t | clk_acc
| Advertiser clock accuracy. More...
gap_bdaddr_t | bd_addr
| Advertiser address. More...
uint16_t | sync_hdl
| Sync handle. More...

## Detailed Description

Sync established indication.

Definition at line 307 of file ble_gapc.h.

## Member Data Documentation

## ◆ adv_sid

uint8_t gap_sync_established_ind_t::adv_sid

Advertising SID.

Definition at line 311 of file ble_gapc.h.

## ◆ bd_addr

gap_bdaddr_t gap_sync_established_ind_t::bd_addr

Advertiser address.

Definition at line 313 of file ble_gapc.h.

## ◆ clk_acc

uint8_t gap_sync_established_ind_t::clk_acc

Advertiser clock accuracy.

See also
  enum gapm_clk_acc.

Definition at line 312 of file ble_gapc.h.

## ◆ intv

uint16_t gap_sync_established_ind_t::intv

Periodic advertising interval (in unit of 1.25ms, min is 7.5ms).

Definition at line 310 of file ble_gapc.h.

## ◆ phy

uint8_t gap_sync_established_ind_t::phy

PHY on which synchronization has been established.

See also
  gap_phy_type.

Definition at line 309 of file ble_gapc.h.

## ◆ sync_hdl

uint16_t gap_sync_established_ind_t::sync_hdl

Sync handle.

Definition at line 314 of file ble_gapc.h.

The documentation for this struct was generated from the following file:

- ble_gapc.h